Gocator API > Go2.Part > Classes > Go2PartHoleRadius > Functions

Gocator 3x00 API | Contents | Reference |

Functions
Functions Legend
Functions

Function | Description
Go2PartHoleRadius_AutoRefRegionEnabled | Reports whether auto reference regions are enabled.
Go2PartHoleRadius_AutoTiltCorrectionEnabled | Reports whether auto tilt correction is enabled.
Go2PartHoleRadius_DecisionMax | Gets the decision threshold maximum value.
Go2PartHoleRadius_DecisionMin | Gets the decision threshold minimum value.
Go2PartHoleRadius_EnableAutoRefRegion | Enables or disables auto reference regions.
Go2PartHoleRadius_EnableAutoTiltCorrection | Enables or disables auto tilt correction.
Go2PartHoleRadius_EnableHold | Enables measurement value hold.
Go2PartHoleRadius_EnableLink | Enables measurement linking. When enabled, another measurement of the same base type can be linked, provided that it is a different measurement(e.g. A Go2PartHoleRadius and Go2PartHoleX measurement can be linked, but you can not link two Go2PartHoleRadius measurements).
Go2PartHoleRadius_EnablePartialDetection | Enables or disables partial hole detection.
Go2PartHoleRadius_EnableRefRegions | Enables or disables the optional reference region.
Go2PartHoleRadius_EnableRegion | Enables or disables the optional region.
Go2PartHoleRadius_EnableSmoothing | Enables measurement value smoothing.
Go2PartHoleRadius_HoldEnabled | Reports whether value hold is currently enabled.
Go2PartHoleRadius_Id | Gets the unique measurement identifier for the measurement.
Go2PartHoleRadius_Link | Gets the measurement id of the linked measurement.
Go2PartHoleRadius_LinkEnabled | Reports whether measurement linking is enabled.
Go2PartHoleRadius_LinkOptionAt | Gets the link-able measurement id at the specified index.
Go2PartHoleRadius_LinkOptionCount | Gets the number of link-able measurement IDs.
Go2PartHoleRadius_Name | Gets the descriptive name for the measurement.
Go2PartHoleRadius_NominalRadius | Gets the nominal radius of the hole to measure.
Go2PartHoleRadius_Offset | Gets the measurement value offset.
Go2PartHoleRadius_PartialDetectionEnabled | Gets the current partial hole detection value.
Go2PartHoleRadius_RadiusTolerance | Gets the tolerance between the nominal radius and the detected hole size.
Go2PartHoleRadius_RefRegionAt | Gets the reference region object at the specified index.
Go2PartHoleRadius_RefRegionCount | Gets the number of reference regions.
Go2PartHoleRadius_RefRegionsEnabled | Returns the current state of the optional reference region.
Go2PartHoleRadius_Region | Gets the region object which defines the measurement's ROI.
Go2PartHoleRadius_RegionEnabled | Returns the current state of the optional region.
Go2PartHoleRadius_Scale | Gets the measurement value scale factor.
Go2PartHoleRadius_SetDecisionMax | Sets the decision threshold maximum value.
Go2PartHoleRadius_SetDecisionMin | Sets the decision threshold minimum value.
Go2PartHoleRadius_SetId | Sets the unique measurement identifier for the measurement.
Go2PartHoleRadius_SetLink | Sets the measurement id to which this measurement should link. Linked measurements must: -link to a valid measurement id -not link to themselves -not link to a measurement that is already linked -link only to measurements of the same basic type (eg, all PartStud_? measurements)
Go2PartHoleRadius_SetName | Sets the descriptive name for the measurement.
Go2PartHoleRadius_SetNominalRadius | Sets the nominal radius of the hole to measure.
Go2PartHoleRadius_SetOffset | Sets the measurement value offset.
Go2PartHoleRadius_SetRadiusTolerance | Sets the tolerance between the nominal radius and the detected hole size.
Go2PartHoleRadius_SetRefRegionCount | Sets the number of reference regions to use.
Go2PartHoleRadius_SetScale | Sets the measurement value scale factor.
Go2PartHoleRadius_SetSmoothingWindow | Sets the smoothing window value.
Go2PartHoleRadius_SetTiltXAngle | Sets the X axis tilt angle.
Go2PartHoleRadius_SetTiltYAngle | Sets the Y axis tilt angle.
Go2PartHoleRadius_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2PartHoleRadius_SmoothingWindow | Gets the smoothing window value.
Go2PartHoleRadius_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2PartHoleRadius_SmoothingWindowMin | Gets the minimum smoothing window value.
Go2PartHoleRadius_TiltXAngle | Gets the X axis tilt angle.
Go2PartHoleRadius_TiltYAngle | Gets the Y axis tilt angle.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference