Gocator API > Go2.Part > Classes > Go2PartHoleX > Functions

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Functions
Functions Go2PartHoleX

Go2PartHoleX Functions

Functions

Function | Description
Go2PartHoleX_AutoRefRegionEnabled | Reports whether auto reference regions are enabled.
Go2PartHoleX_AutoTiltCorrectionEnabled | Reports whether auto tilt correction is enabled.
Go2PartHoleX_DecisionMax | Gets the decision threshold maximum value.
Go2PartHoleX_DecisionMin | Gets the decision threshold minimum value.
Go2PartHoleX_EnableAutoRefRegion | Enables or disables auto reference regions.
Go2PartHoleX_EnableAutoTiltCorrection | Enables or disables auto tilt correction.
Go2PartHoleX_EnableHold | Enables measurement value hold.
Go2PartHoleX_EnableLink | Enables measurement linking. When enabled, another measurement of the same base type can be linked, provided that it is a different measurement.
Go2PartHoleX_EnablePartialDetection | Enable or disable partial hole detection.
Go2PartHoleX_EnableRefRegions | Enables or disables the optional reference region.
Go2PartHoleX_EnableRegion | Enables or disables the optional region.
Go2PartHoleX_EnableSmoothing | Enables measurement value smoothing.
Go2PartHoleX_HoldEnabled | Reports whether value hold is currently enabled.
Go2PartHoleX_Id | Gets the unique measurement identifier for the measurement.
Go2PartHoleX_Link | Gets the measurement id of the linked measurement.
Go2PartHoleX_LinkEnabled | Reports whether bounding box rotation is enabled.
Go2PartHoleX_LinkOptionAt | Gets the link-able measurement id at the specified index.
Go2PartHoleX_LinkOptionCount | Gets the number of link-able measurement IDs.
Go2PartHoleX_Name | Gets the descriptive name for the measurement.
Go2PartHoleX_NominalRadius | Gets the nominal radius of the hole to measure.
Go2PartHoleX_Offset | Gets the measurement value offset.
Go2PartHoleX_PartialDetectionEnabled | Returns the current state of partial hole detection.
Go2PartHoleX_RadiusTolerance | Gets the tolerance between the nominal radius and the detected hole size.
Go2PartHoleX_RefRegionAt | Gets the reference region object at the specified index.
Go2PartHoleX_RefRegionCount | Gets the number of reference regions.
Go2PartHoleX_RefRegionsEnabled | Returns the current state of the optional reference region.
Go2PartHoleX_Region | Gets the region object which defines the measurement's ROI.
Go2PartHoleX_RegionEnabled | Returns the current state of the optional region.
Go2PartHoleX_Scale | Gets the measurement value scale factor.
Go2PartHoleX_SetDecisionMax | Sets the decision threshold maximum value.
Go2PartHoleX_SetDecisionMin | Sets the decision threshold minimum value.
Go2PartHoleX_SetId | Sets the unique measurement identifier for the measurement.
Go2PartHoleX_SetLink | Sets the measurement id to which this measurement should link. Linked measurements must: -link to a valid measurement id -not link to themselves -not link to a measurement that is already linked -link only to measurements of the same basic type (eg, all PartStud_? measurements)
Go2PartHoleX_SetName | Sets the descriptive name for the measurement.
Go2PartHoleX_SetNominalRadius | Sets the nominal radius of the hole to measure.
Go2PartHoleX_SetOffset | Sets the measurement value offset.
Go2PartHoleX_SetRadiusTolerance | Sets the tolerance between the nominal radius and the detected hole size.
Go2PartHoleX_SetRefRegionCount | Sets the number of reference regions to use.
Go2PartHoleX_SetScale | Sets the measurement value scale factor.
Go2PartHoleX_SetSmoothingWindow | Sets the smoothing window value.
Go2PartHoleX_SetTiltXAngle | Sets the X axis tilt angle.
Go2PartHoleX_SetTiltYAngle | Sets the Y axis tilt angle.
Go2PartHoleX_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2PartHoleX_SmoothingWindow | Gets the smoothing window value.
Go2PartHoleX_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2PartHoleX_SmoothingWindowMin | Gets the minimum smoothing window value.
Go2PartHoleX_TiltXAngle | Gets the X axis tilt angle.
Go2PartHoleX_TiltYAngle | Gets the Y axis tilt angle.

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference