Gocator API > Go2 > Classes > Go2System > Functions > Go2System_Connect

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Go2System_Connect
Functions
Description

Connects to a sensor.

C

    Go2Status Go2System_Connect(Go2System system, Go2IPAddress address);

Parameters

Parameters | Description
Go2System system | Go2System object.
Go2IPAddress address | Sensor IP address.

Returns

Operation status.

Remarks

This function assumes that the sensor is ready to accept a connection. But if the sensor has recently been repowered or reset, then this function may timeout. In this case, the Go2System_Reconnect function can be used to wait a reasonable amount of time for a recently repowered or reset sensor to initialize.

File

Go2System.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference