Gocator API > Go2.Profile > Classes > Go2ProfileDifferencePeak > Functions

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Functions
Functions Go2ProfileDifferencePeak
Functions

Function | Description
Go2ProfileDifferencePeak_AbsoluteResult | Gets whether this measurement should calculate absolute measurements.
Go2ProfileDifferencePeak_Area | Gets the region of interest.
Go2ProfileDifferencePeak_DecisionMax | Gets the decision threshold maximum value.
Go2ProfileDifferencePeak_DecisionMin | Gets the decision threshold minimum value.
Go2ProfileDifferencePeak_EnableHold | Enables measurement value hold.
Go2ProfileDifferencePeak_EnableLink | Enables or disables measurement linking.
Go2ProfileDifferencePeak_EnableSmoothing | Enables measurement value smoothing.
Go2ProfileDifferencePeak_HoldEnabled | Reports whether value hold is currently enabled.
Go2ProfileDifferencePeak_Id | Gets the unique measurement identifier for the measurement.
Go2ProfileDifferencePeak_Link | Gets the measurement id of the linked measurement.
Go2ProfileDifferencePeak_LinkEnabled | Enables measurement linking. When enabled, another measurement of the same base type can be linked, provided that it is a different measurement. E.g. A Go2PartOpeningX and Go2PartOpeningY measurement can link, but two Go2PartOpeningX measurements can not be linked.
Go2ProfileDifferencePeak_LinkOptionAt | Gets the link-able measurement id at the specified index.
Go2ProfileDifferencePeak_LinkOptionCount | Gets the number of link-able measurement IDs.
Go2ProfileDifferencePeak_Name | Gets the descriptive name for the measurement.
Go2ProfileDifferencePeak_Offset | Gets the measurement value offset.
Go2ProfileDifferencePeak_Scale | Gets the measurement value scale factor.
Go2ProfileDifferencePeak_SetAbsoluteResult | Sets whether this measurement should calculate absolute measurements. In this case, negative areas (those that fall below the template) would be added to the postive areas to find the total.
Go2ProfileDifferencePeak_SetDecisionMax | Sets the decision threshold maximum value.
Go2ProfileDifferencePeak_SetDecisionMin | Sets the decision threshold minimum value.
Go2ProfileDifferencePeak_SetId | Sets the unique measurement identifier for the measurement.
Go2ProfileDifferencePeak_SetLink | Sets the measurement id to which this measurement should link. Linked measurements must: -link to a valid measurement id -not link to themselves -not link to a measurement that is already linked -link only to measurements of the same basic type (eg, all PartOpening_? measurements)
Go2ProfileDifferencePeak_SetName | Sets the descriptive name for the measurement.
Go2ProfileDifferencePeak_SetOffset | Sets the measurement value offset.
Go2ProfileDifferencePeak_SetScale | Sets the measurement value scale factor.
Go2ProfileDifferencePeak_SetSmoothingWindow | Sets the smoothing window value.
Go2ProfileDifferencePeak_SetSource | Sets the source for profile data used in this measurement.
Go2ProfileDifferencePeak_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2ProfileDifferencePeak_SmoothingWindow | Gets the smoothing window value.
Go2ProfileDifferencePeak_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2ProfileDifferencePeak_SmoothingWindowMin | Gets the minimum smoothing window value.
Go2ProfileDifferencePeak_Source | Gets the source for profile data used in this measurement.
Go2ProfileDifferencePeak_SourceOptionAt | Gets the profile source option at the specified index.
Go2ProfileDifferencePeak_SourceOptionCount | Gets the number of profile source options for the measurement.

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference