Gocator API > Go2.Profile > Values > Go2ProfileGrooveLocation

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2ProfileGrooveLocation
Values
Description

Determines the location of the groove to measure.

C

    enum Go2ProfileGrooveLocation {
      GO2_PROFILE_GROOVE_LOCATION_BOTTOM = 0,
      GO2_PROFILE_GROOVE_LOCATION_LEFT = 1,
      GO2_PROFILE_GROOVE_LOCATION_RIGHT = 2
    };

Members

Members | Description
GO2_PROFILE_GROOVE_LOCATION_BOTTOM = 0 | Measure the bottom of the groove.
GO2_PROFILE_GROOVE_LOCATION_LEFT = 1 | Measure the left corner of the groove.
GO2_PROFILE_GROOVE_LOCATION_RIGHT = 2 | Measure the right corner of the groove.

File

Go2ProfileTypes.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference