Gocator API > Go2.Profile > Values > Go2ProfileStripEdgeType

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2ProfileStripEdgeType
Values
Description

Determines what types of edges are considered valid for this strip.

C

    enum Go2ProfileStripEdgeType {
      GO2_PROFILE_STRIP_EDGE_RISING = 1,
      GO2_PROFILE_STRIP_EDGE_FALLING = 2,
      GO2_PROFILE_STRIP_EDGE_DATA_END = 4,
      GO2_PROFILE_STRIP_EDGE_VOID = 8
    };

Members

Members | Description
GO2_PROFILE_STRIP_EDGE_RISING = 1 | Detect rising edges.
GO2_PROFILE_STRIP_EDGE_FALLING = 2 | Detect falling edges.
GO2_PROFILE_STRIP_EDGE_DATA_END = 4 | Detect edges next to a void in the data.
GO2_PROFILE_STRIP_EDGE_VOID = 8 | Detect edges next to the end of the data.

File

Go2ProfileTypes.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference