Gocator API > Go2.Part > Classes > Go2PartPositionY > Functions > Go2PartPositionY_DecisionMax

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

Go2PartPositionY_DecisionMax
Functions
Description

Gets the decision threshold maximum value.

C

    Go2Double Go2PartPositionY_DecisionMax(Go2PartPositionY measurement);

Parameters

Parameters | Description
Go2PartPositionY measurement | Go2PartPositionY object.

Returns

Decision threshold maximum.

Remarks

A decision is said to pass if the measurement value is between the minimum and maximum thresholds.

File

Go2PartPositionY.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference