Gocator API > Go2.Part > Values > Go2PartFeature3dType

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

Go2PartFeature3dType
Values
Description

Represents the type for a part feature.

C

    enum Go2PartFeature3dType {
      GO2_PART_2D_CENTROID = 0,
      GO2_PART_3D_CENTROID = 1,
      GO2_PART_X_MIN = 2,
      GO2_PART_X_MAX = 3,
      GO2_PART_Y_MIN = 4,
      GO2_PART_Y_MAX = 5,
      GO2_PART_Z_MIN = 6,
      GO2_PART_Z_MAX = 7
    };

Members

Members | Description
GO2_PART_2D_CENTROID = 0 | Find the height for a part at the centroid
GO2_PART_3D_CENTROID = 1 | Find the height for a part at the centroid
GO2_PART_X_MIN = 2 | Find the height for a part at the minimum X position
GO2_PART_X_MAX = 3 | Find the height for a part at the maximum X position
GO2_PART_Y_MIN = 4 | Find the height for a part at the minimum Y position
GO2_PART_Y_MAX = 5 | Find the height for a part at the maximum Y position
GO2_PART_Z_MIN = 6 | Find the height for a part at the minimum Z position
GO2_PART_Z_MAX = 7 | Find the height for a part at the maximum Z position

File

Go2PartTypes.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference