Gocator API > Go2.Output > Classes > Go2Serial > Functions > Go2Serial_AsciiCustomFormatEnabled

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2Serial_AsciiCustomFormatEnabled
Functions
Description

Reports whether the ASCII custom data format is currently enabled. This setting only applies when the operation is asynchronous. When enabled, the measurements selected via add/remove source are ignored.

C

    Go2Bool Go2Serial_AsciiCustomFormatEnabled(Go2Serial serial);

Parameters

Parameters | Description
Go2Serial serial | Go2Serial object.

Returns

GO2_TRUE if enabled, or GO2_FALSE if disabled.

File

Go2OutputChannels.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference