Gocator API > Go2 > Classes > Go2System > Functions > Go2System_ScheduleAnalogOutput

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

Go2System_ScheduleAnalogOutput
Functions
Description

Schedules an analog output. Requires that the output be configured to trigger on software control

C

    Go2Status Go2System_ScheduleAnalogOutput(Go2System system, Go2Analog analog, Go2Int64 target, Go2Int64 value);

Parameters

Parameters | Description
Go2System system | Go2System object.
Go2Analog analog | Go2Analog object.
Go2Int64 target | The time or position target (uS or ticks), depending on Go2System_SystemDomain. Ignored if Go2Analog_ScheduleEnabled is false.
Go2Int64 value | The value of the scheduled output (uA).

Returns

Operation status.

File

Go2System.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference