Gocator API

- Home
- Categories
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Groups Pages
Public Member Functions
GoExposureCalMsg Class Reference
Data Channel

## Description

Represents a message containing exposure calibration results.

Inheritance diagram for GoExposureCalMsg:

## Public Member Functions
GoDataMessageType | GoDataMsg_Type (GoDataMsg message)
| Returns the message type for a data channel message given in a GoDataSet. More...
k32u | GoExposureCalMsg_Exposure (GoExposureCalMsg msg)
| Gets the calibrated exposure. More...
kStatus | GoExposureCalMsg_Status (GoExposureCalMsg msg)
| Gets the exposure calibration result. More...

## Member Function Documentation

GoDataMessageType GoDataMsg_Type | ( | GoDataMsg | message | ) |
| inherited

Returns the message type for a data channel message given in a GoDataSet.

Parameters

  message | A data channel message.

Returns
  A GoDataMessageType value.

k32u GoExposureCalMsg_Exposure | ( | GoExposureCalMsg | msg | ) |

Gets the calibrated exposure.

Parameters

  msg | Message object.

Returns
  Calibrated exposure value in uS.

kStatus GoExposureCalMsg_Status | ( | GoExposureCalMsg | msg | ) |

Gets the exposure calibration result.

Parameters

  msg | Message object.

Returns
  Exposure calibration result.

The documentation for this class was generated from the following file:

- Messages/GoDataTypes.h