Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
Public Member Functions
GoSurfaceMsg Class Reference
GoSdk/Messages » Data Channel

## Description

Represents a data message containing a surface array.

Inheritance diagram for GoSurfaceMsg:

## Public Member Functions
GoDataMessageType | GoDataMsg_Type (GoDataMsg message)
| Returns the message type for a data channel message given in a GoDataSet. More...
k32u | GoSurfaceMsg_Exposure (GoSurfaceMsg msg)
| Gets the exposure. More...
kSize | GoSurfaceMsg_Length (GoSurfaceMsg msg)
| Gets the length of the surface (row count). More...
k16s * | GoSurfaceMsg_RowAt (GoSurfaceMsg msg, kSize index)
| Gets a pointer to a surface row. More...
GoDataSource | GoSurfaceMsg_Source (GoSurfaceMsg msg)
| Gets the profile source. More...
k32u | GoSurfaceMsg_SurfaceId (GoSurfaceMsg msg)
| Gets the surface ID. More...
kSize | GoSurfaceMsg_Width (GoSurfaceMsg msg)
| Gets the width of the surface (column count). More...
k32s | GoSurfaceMsg_XOffset (GoSurfaceMsg msg)
| Gets the surface x-offset, in micrometers. More...
k32u | GoSurfaceMsg_XResolution (GoSurfaceMsg msg)
| Gets the surface x-resolution, in nanometers. More...
k32s | GoSurfaceMsg_YOffset (GoSurfaceMsg msg)
| Gets the surface y-offset, in micrometers. More...
k32u | GoSurfaceMsg_YResolution (GoSurfaceMsg msg)
| Gets the surface y-resolution, in nanometers. More...
k32s | GoSurfaceMsg_ZAngle (GoSurfaceMsg msg)
| Gets the surface z-angle, in microdegrees. More...
k32s | GoSurfaceMsg_ZOffset (GoSurfaceMsg msg)
| Gets the surface z-offset, in micrometers. More...
k32u | GoSurfaceMsg_ZResolution (GoSurfaceMsg msg)
| Gets the surface z-resolution, in nanometers. More...

The documentation for this class was generated from the following file:

- Messages/GoDataTypes.h