Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
GoEthernet.h
Go to the documentation of this file.
1 /**
2 * @file GoEthernet.h
3 * @brief Declares the GoEthernet class.
4 *
5 * @internal
6 * Copyright (C) 2015 by LMI Technologies Inc.
7 * Licensed under the MIT License.
8 * Redistributed files must retain the above copyright notice.
9 */
10 #ifndef GO_SDK_ETHERNET_H
11 #define GO_SDK_ETHERNET_H
12
13 #include <GoSdk/GoSdkDef.h>
14 kBeginHeader()
15
16
17 /**
18 * @class GoEthernet
19 * @extends kObject
20 * @ingroup GoSdk-Ethernet
21 * @brief Represents Ethernet output settings.
22 */
23 typedef kObject GoEthernet;
24
25 /**
26 * Indicates whether the ethernet connection timeout is enabled. If it is
27 * enabled, the configured timeout value will be used.
28 *
29 * @public @memberof GoEthernet
30 * @param ethernet GoEthernet object.
31 * @return kTRUE if enabled and kFALSE otherwise.
32 * @see GoEthernet_Timeout, GoEthernet_SetTimeout
33 */
34 GoFx(kBool) GoEthernet_TimeoutEnabled(GoEthernet ethernet);
35
36 /**
37 * Enables or disables the ethernet connection timeout.
38 *
39 * @public @memberof GoEthernet
40 * @param ethernet GoEthernet object.
41 * @param value kTRUE to enable the connection timeout and
42 * kFALSE to disable it.
43 * @return Operation status.
44 */
45 GoFx(kStatus) GoEthernet_EnableTimeout(GoEthernet ethernet, kBool value);
46
47 /**
48 * Returns the connection timeout value in minutes.
49 *
50 * @public @memberof GoEthernet
51 * @param ethernet GoEthernet object.
52 * @return Connection timeout value in minutes.
53 */
54 GoFx(k64f) GoEthernet_Timeout(GoEthernet ethernet);
55
56 /**
57 * Sets the connection timeout value.
58 *
59 * @public @memberof GoEthernet
60 * @param ethernet GoEthernet object.
61 * @param value The timeout value (in minutes).
62 * @return Operation status.
63 */
64 GoFx(kStatus) GoEthernet_SetTimeout(GoEthernet ethernet, k64f value);
65
66 /**
67 * Gets the number of source options for the specified output type.
68 *
69 * @public @memberof GoEthernet
70 * @version Introduced in firmware 4.0.10.27
71 * @param ethernet GoEthernet object.
72 * @param type Output source type.
73 * @return Count of source options.
74 */
75 GoFx(kSize) GoEthernet_OptionCount(GoEthernet ethernet, GoOutputSource type);
76
77 /**
78 * Gets the source option at the specified index.
79 *
80 * @public @memberof GoEthernet
81 * @version Introduced in firmware 4.0.10.27
82 * @param ethernet GoEthernet object.
83 * @param type Output source type.
84 * @param index Source option index.
85 * @return Source option.
86 */
87 GoFx(k32u) GoEthernet_OptionAt(GoEthernet ethernet, GoOutputSource type, kSize index);
88
89 /**
90 * Gets the number of sources of the specified output type that are currently selected for transmission.
91 *
92 * @public @memberof GoEthernet
93 * @version Introduced in firmware 4.0.10.27
94 * @param ethernet GoEthernet object.
95 * @param type Output source type.
96 * @return Count of selected sources.
97 */
98 GoFx(kSize) GoEthernet_SourceCount(GoEthernet ethernet, GoOutputSource type);
99
100 /**
101 * Gets the identifier of the selected output at the specified index.
102 *
103 * @public @memberof GoEthernet
104 * @version Introduced in firmware 4.0.10.27
105 * @param ethernet GoEthernet object.
106 * @param type Output source type.
107 * @param index Selected source index.
108 * @return Source identifier.
109 */
110 GoFx(k32u) GoEthernet_SourceAt(GoEthernet ethernet, GoOutputSource type, kSize index);
111
112 /**
113 * Selects the specified source for transmission.
114 *
115 * @public @memberof GoEthernet
116 * @version Introduced in firmware 4.0.10.27
117 * @param ethernet GoEthernet object.
118 * @param type Output source type.
119 * @param sourceId Output source identifier.
120 * @return Operation status.
121 */
122 GoFx(kStatus) GoEthernet_AddSource(GoEthernet ethernet, GoOutputSource type, k32u sourceId);
123
124 /**
125 * Removes (deselects) the source at the specified index.
126 *
127 * @public @memberof GoEthernet
128 * @version Introduced in firmware 4.0.10.27
129 * @param ethernet GoEthernet object.
130 * @param type Output source type.
131 * @param index Index of the source to be removed.
132 * @return Operation status.
133 */
134 GoFx(kStatus) GoEthernet_RemoveSource(GoEthernet ethernet, GoOutputSource type, kSize index);
135
136 /**
137 * Removes (deselects) all selected sources for the specified output type.
138 *
139 * @public @memberof GoEthernet
140 * @version Introduced in firmware 4.0.10.27
141 * @param ethernet GoEthernet object.
142 * @param type Output source type.
143 * @return Operation status.
144 */
145 GoFx(kStatus) GoEthernet_ClearSources(GoEthernet ethernet, GoOutputSource type);
146
147 /**
148 * Removes (deselects) all selected sources for all possible ethernet output types.
149 *
150 * @public @memberof GoEthernet
151 * @version Introduced in firmware 4.0.10.27
152 * @param ethernet GoEthernet object.
153 * @return Operation status.
154 */
155 GoFx(kStatus) GoEthernet_ClearAllSources(GoEthernet ethernet);
156
157 /**
158 * Gets the protocol that the ethernet utilizes for output.
159 *
160 * @public @memberof GoEthernet
161 * @version Introduced in firmware 4.0.10.27
162 * @param ethernet GoEthernet object.
163 * @return The ethernet protocol.
164 */
165 GoFx(GoEthernetProtocol) GoEthernet_Protocol(GoEthernet ethernet);
166
167 /**
168 * Sets the protocol which will be output via ethernet.
169 *
170 * @public @memberof GoEthernet
171 * @version Introduced in firmware 4.0.10.27
172 * @param ethernet GoEthernet object.
173 * @param protocol The selected ethernet protocol.
174 * @return Operation status.
175 */
176 GoFx(kStatus) GoEthernet_SetProtocol(GoEthernet ethernet, GoEthernetProtocol protocol);
177
178 /**
179 * Gets the ASCII protocol operational mode.
180 *
181 * @public @memberof GoEthernet
182 * @version Introduced in firmware 4.0.10.27
183 * @param ethernet GoEthernet object.
184 * @return Operation mode.
185 */
186 GoFx(GoAsciiOperation) GoEthernet_AsciiOperation(GoEthernet ethernet);
187
188 /**
189 * Sets the ASCII operation mode.
190 *
191 * @public @memberof GoEthernet
192 * @version Introduced in firmware 4.0.10.27
193 * @param ethernet GoEthernet object.
194 * @param mode The selected ASCII operation mode.
195 * @return Operation status.
196 */
197 GoFx(kStatus) GoEthernet_SetAsciiOperation(GoEthernet ethernet, GoAsciiOperation mode);
198
199 /**
200 * Gets the ASCII protocol control channel port number.
201 *
202 * @public @memberof GoEthernet
203 * @version Introduced in firmware 4.0.10.27
204 * @param ethernet GoEthernet object.
205 * @return Control channel port number.
206 */
207 GoFx(k32u) GoEthernet_AsciiControlPort(GoEthernet ethernet);
208
209 /**
210 * Sets the port number of the ASCII control port.
211 *
212 * @public @memberof GoEthernet
213 * @version Introduced in firmware 4.0.10.27
214 * @param ethernet GoEthernet object.
215 * @param port The selected ASCII control port value.
216 * @return Operation status.
217 */
218 GoFx(kStatus) GoEthernet_SetAsciiControlPort(GoEthernet ethernet, k32u port);
219
220 /**
221 * Gets the ASCII protocol health channel port number.
222 *
223 * @public @memberof GoEthernet
224 * @version Introduced in firmware 4.0.10.27
225 * @param ethernet GoEthernet object.
226 * @return Health channel port number.
227 */
228 GoFx(k32u) GoEthernet_AsciiHealthPort(GoEthernet ethernet);
229
230 /**
231 * Sets the port number of the ASCII health port.
232 *
233 * @public @memberof GoEthernet
234 * @version Introduced in firmware 4.0.10.27
235 * @param ethernet GoEthernet object.
236 * @param port The selected ASCII health port value.
237 * @return Operation status.
238 */
239 GoFx(kStatus) GoEthernet_SetAsciiHealthPort(GoEthernet ethernet, k32u port);
240
241 /**
242 * Gets the ASCII protocol data channel port number.
243 *
244 * @public @memberof GoEthernet
245 * @version Introduced in firmware 4.0.10.27
246 * @param ethernet GoEthernet object.
247 * @return Data channel port number.
248 */
249 GoFx(k32u) GoEthernet_AsciiDataPort(GoEthernet ethernet);
250
251 /**
252 * Sets the port number of the ASCII data port.
253 *
254 * @public @memberof GoEthernet
255 * @version Introduced in firmware 4.0.10.27
256 * @param ethernet GoEthernet object.
257 * @param port The selected ASCII data port value.
258 * @return Operation status.
259 */
260 GoFx(kStatus) GoEthernet_SetAsciiDataPort(GoEthernet ethernet, k32u port);
261
262 /**
263 * Gets the ASCII protocol output delimiter string.
264 *
265 * @public @memberof GoEthernet
266 * @version Introduced in firmware 4.0.10.27
267 * @param ethernet GoEthernet object.
268 * @return A pointer to the string representing the ASCII protocol output delimiter.
269 */
270 GoFx(kChar*) GoEthernet_AsciiDelimiter(GoEthernet ethernet);
271
272 /**
273 * Sets the ASCII protocol output delimiter string.
274 *
275 * @public @memberof GoEthernet
276 * @version Introduced in firmware 4.0.10.27
277 * @param ethernet GoEthernet object.
278 * @param string A pointer to the string representing the ASCII protocol output delimiter.
279 * @return Operation status.
280 */
281 GoFx(kStatus) GoEthernet_SetAsciiDelimiter(GoEthernet ethernet, const kChar* string);
282
283 /**
284 * Gets the ASCII protocol output terminator string.
285 *
286 * @public @memberof GoEthernet
287 * @version Introduced in firmware 4.0.10.27
288 * @param ethernet GoEthernet object.
289 * @return A pointer to the terminator representing the ASCII protocol output delimiter.
290 */
291 GoFx(kChar*) GoEthernet_AsciiTerminator(GoEthernet ethernet);
292
293 /**
294 * Sets the ASCII protocol output terminator string.
295 *
296 * @public @memberof GoEthernet
297 * @version Introduced in firmware 4.0.10.27
298 * @param ethernet GoEthernet object.
299 * @param string A pointer to the string representing the ASCII protocol output terminator.
300 * @return Operation status.
301 */
302 GoFx(kStatus) GoEthernet_SetAsciiTerminator(GoEthernet ethernet, const kChar* string);
303
304 /**
305 * Gets the ASCII protocol output invalid value string.
306 *
307 * @public @memberof GoEthernet
308 * @version Introduced in firmware 4.0.10.27
309 * @param ethernet GoEthernet object.
310 * @return A pointer to the string representing the ASCII protocol output invalid value.
311 */
312 GoFx(kChar*) GoEthernet_AsciiInvalidValue(GoEthernet ethernet);
313
314 /**
315 * Sets the ASCII protocol output invalid value string.
316 *
317 * @public @memberof GoEthernet
318 * @version Introduced in firmware 4.0.10.27
319 * @param ethernet GoEthernet object.
320 * @param string A pointer to the string representing the ASCII protocol output invalid value.
321 * @return Operation status.
322 */
323 GoFx(kStatus) GoEthernet_SetAsciiInvalidValue(GoEthernet ethernet, const kChar* string);
324
325 /**
326 * Gets the ASCII protocol output custom data format string.
327 *
328 * @public @memberof GoEthernet
329 * @version Introduced in firmware 4.0.10.27
330 * @param ethernet GoEthernet object.
331 * @return A pointer to the string representing the ASCII protocol output custom data format.
332 */
333 GoFx(kChar*) GoEthernet_AsciiCustomDataFormat(GoEthernet ethernet);
334
335 /**
336 * Sets the ASCII protocol output custom data format string.
337 *
338 * @public @memberof GoEthernet
339 * @version Introduced in firmware 4.0.10.27
340 * @param ethernet GoEthernet object.
341 * @param string A pointer to the string representing the ASCII protocol output custom data format.
342 * @return Operation status.
343 */
344 GoFx(kStatus) GoEthernet_SetAsciiCustomDataFormat(GoEthernet ethernet, const kChar* string);
345
346 /**
347 * Enables or disables the ASCII protocol output custom data format.
348 *
349 * @public @memberof GoEthernet
350 * @version Introduced in firmware 4.0.10.27
351 * @param ethernet GoEthernet object.
352 * @param enabled kTRUE to enable custom data format output. kFALSE to use the default output format.
353 * @return Operation status.
354 */
355 GoFx(kStatus) GoEthernet_EnableAsciiCustomFormat(GoEthernet ethernet, kBool enabled);
356
357 /**
358 * Returns the value of whether the ASCII protocol custom data format is enabled or disabled.
359 *
360 * @public @memberof GoEthernet
361 * @version Introduced in firmware 4.0.10.27
362 * @param ethernet GoEthernet object.
363 * @return kTRUE if the custom data format is enabled. kFALSE otherwise.
364 */
365 GoFx(kBool) GoEthernet_AsciiCustomFormatEnabled(GoEthernet ethernet);
366
367 /**
368 * Enables or disables EthernetIP protocol output buffering.
369 *
370 * @public @memberof GoEthernet
371 * @version Introduced in firmware 4.0.10.27
372 * @param ethernet GoEthernet object.
373 * @param enabled kTRUE to enable buffering. kFALSE to disable it.
374 * @return Operation status.
375 */
376 GoFx(kStatus) GoEthernet_SetEIPBufferingEnabled(GoEthernet ethernet, kBool enabled);
377
378 /**
379 * Returns the value of whether the EthernetIP protocol output buffering is enabled or disabled.
380 *
381 * @public @memberof GoEthernet
382 * @version Introduced in firmware 4.0.10.27
383 * @param ethernet GoEthernet object.
384 * @return kTRUE if buffering is enabled. kFALSE otherwise.
385 */
386 GoFx(kBool) GoEthernet_EIPBufferingEnabled(GoEthernet ethernet);
387
388 /**
389 * Sets the EthernetIP protocol endian output type.
390 *
391 * @public @memberof GoEthernet
392 * @version Introduced in firmware 4.1.3.106
393 * @param ethernet GoEthernet object.
394 * @param type The endian output type to set.
395 * @return Operation status.
396 */
397 GoFx(kStatus) GoEthernet_SetEIPEndianOutputType(GoEthernet ethernet, GoEndianType type);
398
399 /**
400 * Returns the value of the EthernetIP protocol endian output type.
401 *
402 * @public @memberof GoEthernet
403 * @version Introduced in firmware 4.1.3.106
404 * @param ethernet GoEthernet object.
405 * @return Endian output type.
406 */
407 GoFx(kBool) GoEthernet_EIPEndianOutputType(GoEthernet ethernet);
408
409 /**
410 * Sets the EthernetIP protocol implicit trigger override.
411 *
412 * @public @memberof GoEthernet
413 * @version Introduced in firmware 4.2.4.7
414 * @param ethernet GoEthernet object.
415 * @param value The implicit trigger override value to set.
416 * @return Operation status.
417 */
418 GoFx(kStatus) GoEthernet_SetEIPImplicitTriggerOverride(GoEthernet ethernet, GoImplicitTriggerOverride value);
419
420 /**
421 * Returns the value of the EthernetIP protocol implicit trigger override.
422 *
423 * @public @memberof GoEthernet
424 * @version Introduced in firmware 4.2.4.7
425 * @param ethernet GoEthernet object.
426 * @return Implicit trigger override value.
427 */
428 GoFx(GoImplicitTriggerOverride) GoEthernet_EIPImplicitTriggerOverride(GoEthernet ethernet);
429
430 /**
431 * Enables or disables Modbus protocol output buffering.
432 *
433 * @public @memberof GoEthernet
434 * @version Introduced in firmware 4.0.10.27
435 * @param ethernet GoEthernet object.
436 * @param enabled kTRUE to enable buffering. kFALSE to disable it.
437 * @return Operation status.
438 */
439 GoFx(kStatus) GoEthernet_SetModbusBufferingEnabled(GoEthernet ethernet, kBool enabled);
440
441 /**
442 * Returns the value of whether Modbus protocol output buffering is enabled or disabled.
443 *
444 * @public @memberof GoEthernet
445 * @version Introduced in firmware 4.0.10.27
446 * @param ethernet GoEthernet object.
447 * @return kTRUE if buffering is enabled. kFALSE otherwise.
448 */
449 GoFx(kBool) GoEthernet_ModbusBufferingEnabled(GoEthernet ethernet);
450
451 kEndHeader()
452 #include <GoSdk/Outputs/GoEthernet.x.h>
453
454 #endif
k32u
GoEthernet::GoEthernet_ClearAllSources
kStatus GoEthernet_ClearAllSources(GoEthernet ethernet)
Removes (deselects) all selected sources for all possible ethernet output types.
GoEthernet::GoEthernet_SetEIPImplicitTriggerOverride
kStatus GoEthernet_SetEIPImplicitTriggerOverride(GoEthernet ethernet, GoImplicitTriggerOverride value)
Sets the EthernetIP protocol implicit trigger override.
GoEthernet::GoEthernet_AsciiCustomDataFormat
kChar * GoEthernet_AsciiCustomDataFormat(GoEthernet ethernet)
Gets the ASCII protocol output custom data format string.
GoEthernet::GoEthernet_ModbusBufferingEnabled
kBool GoEthernet_ModbusBufferingEnabled(GoEthernet ethernet)
Returns the value of whether Modbus protocol output buffering is enabled or disabled.
GoEthernet::GoEthernet_RemoveSource
kStatus GoEthernet_RemoveSource(GoEthernet ethernet, GoOutputSource type, kSize index)
Removes (deselects) the source at the specified index.
GoEthernet::GoEthernet_AsciiDataPort
k32u GoEthernet_AsciiDataPort(GoEthernet ethernet)
Gets the ASCII protocol data channel port number.
kSize
GoEthernet::GoEthernet_AsciiControlPort
k32u GoEthernet_AsciiControlPort(GoEthernet ethernet)
Gets the ASCII protocol control channel port number.
GoEthernet::GoEthernet_SetProtocol
kStatus GoEthernet_SetProtocol(GoEthernet ethernet, GoEthernetProtocol protocol)
Sets the protocol which will be output via ethernet.
GoEthernet::GoEthernet_SetAsciiHealthPort
kStatus GoEthernet_SetAsciiHealthPort(GoEthernet ethernet, k32u port)
Sets the port number of the ASCII health port.
GoEthernet::GoEthernet_SetAsciiDelimiter
kStatus GoEthernet_SetAsciiDelimiter(GoEthernet ethernet, const kChar *string)
Sets the ASCII protocol output delimiter string.
GoEthernetProtocol
Represents a ethernet output protocol.
GoEthernet::GoEthernet_TimeoutEnabled
kBool GoEthernet_TimeoutEnabled(GoEthernet ethernet)
Indicates whether the ethernet connection timeout is enabled.
GoEndianType
Represents an endian output type.
kChar
GoEthernet::GoEthernet_EIPImplicitTriggerOverride
GoImplicitTriggerOverride GoEthernet_EIPImplicitTriggerOverride(GoEthernet ethernet)
Returns the value of the EthernetIP protocol implicit trigger override.
GoEthernet::GoEthernet_AsciiDelimiter
kChar * GoEthernet_AsciiDelimiter(GoEthernet ethernet)
Gets the ASCII protocol output delimiter string.
GoEthernet::GoEthernet_SetAsciiCustomDataFormat
kStatus GoEthernet_SetAsciiCustomDataFormat(GoEthernet ethernet, const kChar *string)
Sets the ASCII protocol output custom data format string.
GoEthernet::GoEthernet_SetAsciiInvalidValue
kStatus GoEthernet_SetAsciiInvalidValue(GoEthernet ethernet, const kChar *string)
Sets the ASCII protocol output invalid value string.
GoEthernet::GoEthernet_Timeout
k64f GoEthernet_Timeout(GoEthernet ethernet)
Returns the connection timeout value in minutes.
GoEthernet::GoEthernet_SetAsciiControlPort
kStatus GoEthernet_SetAsciiControlPort(GoEthernet ethernet, k32u port)
Sets the port number of the ASCII control port.
GoEthernet::GoEthernet_AsciiOperation
GoAsciiOperation GoEthernet_AsciiOperation(GoEthernet ethernet)
Gets the ASCII protocol operational mode.
GoEthernet::GoEthernet_AddSource
kStatus GoEthernet_AddSource(GoEthernet ethernet, GoOutputSource type, k32u sourceId)
Selects the specified source for transmission.
GoSdkDef.h
Essential SDK declarations.
GoEthernet::GoEthernet_EnableTimeout
kStatus GoEthernet_EnableTimeout(GoEthernet ethernet, kBool value)
Enables or disables the ethernet connection timeout.
GoEthernet::GoEthernet_AsciiHealthPort
k32u GoEthernet_AsciiHealthPort(GoEthernet ethernet)
Gets the ASCII protocol health channel port number.
GoImplicitTriggerOverride
Represents an EthernetIP implicit messaging trigger override.
GoEthernet::GoEthernet_ClearSources
kStatus GoEthernet_ClearSources(GoEthernet ethernet, GoOutputSource type)
Removes (deselects) all selected sources for the specified output type.
GoEthernet::GoEthernet_SetTimeout
kStatus GoEthernet_SetTimeout(GoEthernet ethernet, k64f value)
Sets the connection timeout value.
GoOutputSource
Represents output sources.
GoEthernet::GoEthernet_EnableAsciiCustomFormat
kStatus GoEthernet_EnableAsciiCustomFormat(GoEthernet ethernet, kBool enabled)
Enables or disables the ASCII protocol output custom data format.
GoEthernet::GoEthernet_Protocol
GoEthernetProtocol GoEthernet_Protocol(GoEthernet ethernet)
Gets the protocol that the ethernet utilizes for output.
GoAsciiOperation
Represents an ASCII protocol operational type.
GoEthernet::GoEthernet_SetEIPBufferingEnabled
kStatus GoEthernet_SetEIPBufferingEnabled(GoEthernet ethernet, kBool enabled)
Enables or disables EthernetIP protocol output buffering.
GoEthernet::GoEthernet_OptionAt
k32u GoEthernet_OptionAt(GoEthernet ethernet, GoOutputSource type, kSize index)
Gets the source option at the specified index.
GoEthernet::GoEthernet_SetAsciiTerminator
kStatus GoEthernet_SetAsciiTerminator(GoEthernet ethernet, const kChar *string)
Sets the ASCII protocol output terminator string.
GoEthernet::GoEthernet_SetAsciiOperation
kStatus GoEthernet_SetAsciiOperation(GoEthernet ethernet, GoAsciiOperation mode)
Sets the ASCII operation mode.
kObject
kStatus
GoEthernet::GoEthernet_SourceAt
k32u GoEthernet_SourceAt(GoEthernet ethernet, GoOutputSource type, kSize index)
Gets the identifier of the selected output at the specified index.
GoEthernet::GoEthernet_SetModbusBufferingEnabled
kStatus GoEthernet_SetModbusBufferingEnabled(GoEthernet ethernet, kBool enabled)
Enables or disables Modbus protocol output buffering.
GoEthernet::GoEthernet_EIPEndianOutputType
kBool GoEthernet_EIPEndianOutputType(GoEthernet ethernet)
Returns the value of the EthernetIP protocol endian output type.
k64f
GoEthernet::GoEthernet_SetEIPEndianOutputType
kStatus GoEthernet_SetEIPEndianOutputType(GoEthernet ethernet, GoEndianType type)
Sets the EthernetIP protocol endian output type.
GoEthernet::GoEthernet_SetAsciiDataPort
kStatus GoEthernet_SetAsciiDataPort(GoEthernet ethernet, k32u port)
Sets the port number of the ASCII data port.
GoEthernet
Represents Ethernet output settings.
kBool
GoEthernet::GoEthernet_EIPBufferingEnabled
kBool GoEthernet_EIPBufferingEnabled(GoEthernet ethernet)
Returns the value of whether the EthernetIP protocol output buffering is enabled or disabled...
GoEthernet::GoEthernet_SourceCount
kSize GoEthernet_SourceCount(GoEthernet ethernet, GoOutputSource type)
Gets the number of sources of the specified output type that are currently selected for transmission...
GoEthernet::GoEthernet_OptionCount
kSize GoEthernet_OptionCount(GoEthernet ethernet, GoOutputSource type)
Gets the number of source options for the specified output type.
GoEthernet::GoEthernet_AsciiCustomFormatEnabled
kBool GoEthernet_AsciiCustomFormatEnabled(GoEthernet ethernet)
Returns the value of whether the ASCII protocol custom data format is enabled or disabled.
GoEthernet::GoEthernet_AsciiTerminator
kChar * GoEthernet_AsciiTerminator(GoEthernet ethernet)
Gets the ASCII protocol output terminator string.
GoEthernet::GoEthernet_AsciiInvalidValue
kChar * GoEthernet_AsciiInvalidValue(GoEthernet ethernet)
Gets the ASCII protocol output invalid value string.