Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoControl_GetAutoStartEnabled | ( | GoControl | control,
|  | kBool * | enabled
| ) |  |

Returns the state of sensor AutoStart.

Version
  Introduced in firmware 4.0.10.27

Parameters

  control | GoControl object.
  enabled | A pointer to store the boolean state of sensor AutoStart. kTRUE if enabled and kFALSE if disabled.

Returns
  Operation status.