Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
Public Member Functions
GoProfileMsg Class Reference
GoSdk/Messages » Data Channel

## Description

Represents a data message containing a set of profile arrays.

Inheritance diagram for GoProfileMsg:

## Public Member Functions
GoDataMessageType | GoDataMsg_Type (GoDataMsg message)
| Returns the message type for a data channel message given in a GoDataSet. More...
k8u | GoProfileIntensityMsg_CameraIndex (GoProfileMsg msg)
| Gets the source camera index. More...
kPoint16s * | GoProfileMsg_At (GoProfileMsg msg, kSize index)
| Gets a pointer to a profile array. More...
k8u | GoProfileMsg_CameraIndex (GoProfileMsg msg)
| Gets the source camera index. More...
kSize | GoProfileMsg_Count (GoProfileMsg msg)
| Gets the count of profile arrays in this message. More...
k32u | GoProfileMsg_Exposure (GoProfileMsg msg)
| Gets the exposure. More...
GoDataSource | GoProfileMsg_Source (GoProfileMsg msg)
| Gets the profile source. More...
kSize | GoProfileMsg_Width (GoProfileMsg msg)
| Gets the count of ranges in each profile array. More...
k32s | GoProfileMsg_XOffset (GoProfileMsg msg)
| Gets the profile x-offset, in micrometers. More...
k32u | GoProfileMsg_XResolution (GoProfileMsg msg)
| Gets the profile x-resolution, in nanometers. More...
k32s | GoProfileMsg_ZOffset (GoProfileMsg msg)
| Gets the profile z-offset, in micrometers. More...
k32u | GoProfileMsg_ZResolution (GoProfileMsg msg)
| Gets the profile z-resolution, in nanometers. More...

The documentation for this class was generated from the following file:

- Messages/GoDataTypes.h