Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSystem_ScheduledStart | ( | GoSystem | system,
|  | k64s | value
| ) |  |

Starts all sensors that are currently in the ready state at a scheduled value.

Version
  Introduced in firmware 4.1.3.106

Parameters

  system | GoSystem object.
  value | The value at which to start the sensor. It is in uS when time triggered and ticks when encoder triggered.

Returns
  Operation status.

See also
  GoSystem_Stop, GoSensor_ScheduledStart, GoSensor_Stop, GoSetup_SetTriggerSource, GoSetup_TriggerSource