Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
GoEthernet.h
Go to the documentation of this file.
1 /**
2 * @file GoEthernet.h
3 * @brief Declares the GoEthernet class.
4 *
5 * @internal
6 * Copyright (C) 2015 by LMI Technologies Inc.
7 * Licensed under the MIT License.
8 * Redistributed files must retain the above copyright notice.
9 */
10 #ifndef GO_SDK_ETHERNET_H
11 #define GO_SDK_ETHERNET_H
12
13 #include <GoSdk/GoSdkDef.h>
14 kBeginHeader()
15
16
17 /**
18 * @class GoEthernet
19 * @extends kObject
20 * @ingroup GoSdk-Ethernet
21 * @brief Represents Ethernet output settings.
22 */
23 typedef kObject GoEthernet;
24
25 /**
26 * Indicates whether the ethernet connection timeout is enabled. If it is
27 * enabled, the configured timeout value will be used.
28 *
29 * @public @memberof GoEthernet
30 * @version Introduced in firmware 4.3.3.124
31 * @param ethernet GoEthernet object.
32 * @return kTRUE if enabled and kFALSE otherwise.
33 * @see GoEthernet_Timeout, GoEthernet_SetTimeout
34 */
35 GoFx(kBool) GoEthernet_TimeoutEnabled(GoEthernet ethernet);
36
37 /**
38 * Enables or disables the ethernet connection timeout.
39 *
40 * @public @memberof GoEthernet
41 * @version Introduced in firmware 4.3.3.124
42 * @param ethernet GoEthernet object.
43 * @param value kTRUE to enable the connection timeout and
44 * kFALSE to disable it.
45 * @return Operation status.
46 */
47 GoFx(kStatus) GoEthernet_EnableTimeout(GoEthernet ethernet, kBool value);
48
49 /**
50 * Returns the connection timeout value in minutes.
51 *
52 * @public @memberof GoEthernet
53 * @version Introduced in firmware 4.3.3.124
54 * @param ethernet GoEthernet object.
55 * @return Connection timeout value in minutes.
56 */
57 GoFx(k64f) GoEthernet_Timeout(GoEthernet ethernet);
58
59 /**
60 * Sets the connection timeout value.
61 *
62 * @public @memberof GoEthernet
63 * @version Introduced in firmware 4.3.3.124
64 * @param ethernet GoEthernet object.
65 * @param value The timeout value (in minutes).
66 * @return Operation status.
67 */
68 GoFx(kStatus) GoEthernet_SetTimeout(GoEthernet ethernet, k64f value);
69
70 /**
71 * Gets the number of source options for the specified output type.
72 *
73 * @public @memberof GoEthernet
74 * @version Introduced in firmware 4.0.10.27
75 * @param ethernet GoEthernet object.
76 * @param type Output source type.
77 * @return Count of source options.
78 */
79 GoFx(kSize) GoEthernet_OptionCount(GoEthernet ethernet, GoOutputSource type);
80
81 /**
82 * Gets the source option at the specified index.
83 *
84 * @public @memberof GoEthernet
85 * @version Introduced in firmware 4.0.10.27
86 * @param ethernet GoEthernet object.
87 * @param type Output source type.
88 * @param index Source option index.
89 * @return Source option.
90 */
91 GoFx(k32u) GoEthernet_OptionAt(GoEthernet ethernet, GoOutputSource type, kSize index);
92
93 /**
94 * Gets the number of sources of the specified output type that are currently selected for transmission.
95 *
96 * @public @memberof GoEthernet
97 * @version Introduced in firmware 4.0.10.27
98 * @param ethernet GoEthernet object.
99 * @param type Output source type.
100 * @return Count of selected sources.
101 */
102 GoFx(kSize) GoEthernet_SourceCount(GoEthernet ethernet, GoOutputSource type);
103
104 /**
105 * Gets the identifier of the selected output at the specified index.
106 *
107 * @public @memberof GoEthernet
108 * @version Introduced in firmware 4.0.10.27
109 * @param ethernet GoEthernet object.
110 * @param type Output source type.
111 * @param index Selected source index.
112 * @return Source identifier.
113 */
114 GoFx(k32u) GoEthernet_SourceAt(GoEthernet ethernet, GoOutputSource type, kSize index);
115
116 /**
117 * Selects the specified source for transmission.
118 *
119 * @public @memberof GoEthernet
120 * @version Introduced in firmware 4.0.10.27
121 * @param ethernet GoEthernet object.
122 * @param type Output source type.
123 * @param sourceId Output source identifier.
124 * @return Operation status.
125 */
126 GoFx(kStatus) GoEthernet_AddSource(GoEthernet ethernet, GoOutputSource type, k32u sourceId);
127
128 /**
129 * Removes (deselects) the source at the specified index.
130 *
131 * @public @memberof GoEthernet
132 * @version Introduced in firmware 4.0.10.27
133 * @param ethernet GoEthernet object.
134 * @param type Output source type.
135 * @param index Index of the source to be removed.
136 * @return Operation status.
137 */
138 GoFx(kStatus) GoEthernet_RemoveSource(GoEthernet ethernet, GoOutputSource type, kSize index);
139
140 /**
141 * Removes (deselects) all selected sources for the specified output type.
142 *
143 * @public @memberof GoEthernet
144 * @version Introduced in firmware 4.0.10.27
145 * @param ethernet GoEthernet object.
146 * @param type Output source type.
147 * @return Operation status.
148 */
149 GoFx(kStatus) GoEthernet_ClearSources(GoEthernet ethernet, GoOutputSource type);
150
151 /**
152 * Removes (deselects) all selected sources for all possible ethernet output types.
153 *
154 * @public @memberof GoEthernet
155 * @version Introduced in firmware 4.0.10.27
156 * @param ethernet GoEthernet object.
157 * @return Operation status.
158 */
159 GoFx(kStatus) GoEthernet_ClearAllSources(GoEthernet ethernet);
160
161 /**
162 * Gets the protocol that the ethernet utilizes for output.
163 *
164 * @public @memberof GoEthernet
165 * @version Introduced in firmware 4.0.10.27
166 * @param ethernet GoEthernet object.
167 * @return The ethernet protocol.
168 */
169 GoFx(GoEthernetProtocol) GoEthernet_Protocol(GoEthernet ethernet);
170
171 /**
172 * Sets the protocol which will be output via ethernet.
173 *
174 * @public @memberof GoEthernet
175 * @version Introduced in firmware 4.0.10.27
176 * @param ethernet GoEthernet object.
177 * @param protocol The selected ethernet protocol.
178 * @return Operation status.
179 */
180 GoFx(kStatus) GoEthernet_SetProtocol(GoEthernet ethernet, GoEthernetProtocol protocol);
181
182 /**
183 * Gets the ASCII protocol operational mode.
184 *
185 * @public @memberof GoEthernet
186 * @version Introduced in firmware 4.0.10.27
187 * @param ethernet GoEthernet object.
188 * @return Operation mode.
189 */
190 GoFx(GoAsciiOperation) GoEthernet_AsciiOperation(GoEthernet ethernet);
191
192 /**
193 * Sets the ASCII operation mode.
194 *
195 * @public @memberof GoEthernet
196 * @version Introduced in firmware 4.0.10.27
197 * @param ethernet GoEthernet object.
198 * @param mode The selected ASCII operation mode.
199 * @return Operation status.
200 */
201 GoFx(kStatus) GoEthernet_SetAsciiOperation(GoEthernet ethernet, GoAsciiOperation mode);
202
203 /**
204 * Gets the ASCII protocol control channel port number.
205 *
206 * @public @memberof GoEthernet
207 * @version Introduced in firmware 4.0.10.27
208 * @param ethernet GoEthernet object.
209 * @return Control channel port number.
210 */
211 GoFx(k32u) GoEthernet_AsciiControlPort(GoEthernet ethernet);
212
213 /**
214 * Sets the port number of the ASCII control port.
215 *
216 * @public @memberof GoEthernet
217 * @version Introduced in firmware 4.0.10.27
218 * @param ethernet GoEthernet object.
219 * @param port The selected ASCII control port value.
220 * @return Operation status.
221 */
222 GoFx(kStatus) GoEthernet_SetAsciiControlPort(GoEthernet ethernet, k32u port);
223
224 /**
225 * Gets the ASCII protocol health channel port number.
226 *
227 * @public @memberof GoEthernet
228 * @version Introduced in firmware 4.0.10.27
229 * @param ethernet GoEthernet object.
230 * @return Health channel port number.
231 */
232 GoFx(k32u) GoEthernet_AsciiHealthPort(GoEthernet ethernet);
233
234 /**
235 * Sets the port number of the ASCII health port.
236 *
237 * @public @memberof GoEthernet
238 * @version Introduced in firmware 4.0.10.27
239 * @param ethernet GoEthernet object.
240 * @param port The selected ASCII health port value.
241 * @return Operation status.
242 */
243 GoFx(kStatus) GoEthernet_SetAsciiHealthPort(GoEthernet ethernet, k32u port);
244
245 /**
246 * Gets the ASCII protocol data channel port number.
247 *
248 * @public @memberof GoEthernet
249 * @version Introduced in firmware 4.0.10.27
250 * @param ethernet GoEthernet object.
251 * @return Data channel port number.
252 */
253 GoFx(k32u) GoEthernet_AsciiDataPort(GoEthernet ethernet);
254
255 /**
256 * Sets the port number of the ASCII data port.
257 *
258 * @public @memberof GoEthernet
259 * @version Introduced in firmware 4.0.10.27
260 * @param ethernet GoEthernet object.
261 * @param port The selected ASCII data port value.
262 * @return Operation status.
263 */
264 GoFx(kStatus) GoEthernet_SetAsciiDataPort(GoEthernet ethernet, k32u port);
265
266 /**
267 * Gets the ASCII protocol output delimiter string.
268 *
269 * @public @memberof GoEthernet
270 * @version Introduced in firmware 4.0.10.27
271 * @param ethernet GoEthernet object.
272 * @return A pointer to the string representing the ASCII protocol output delimiter.
273 */
274 GoFx(kChar*) GoEthernet_AsciiDelimiter(GoEthernet ethernet);
275
276 /**
277 * Sets the ASCII protocol output delimiter string.
278 *
279 * @public @memberof GoEthernet
280 * @version Introduced in firmware 4.0.10.27
281 * @param ethernet GoEthernet object.
282 * @param string A pointer to the string representing the ASCII protocol output delimiter.
283 * @return Operation status.
284 */
285 GoFx(kStatus) GoEthernet_SetAsciiDelimiter(GoEthernet ethernet, const kChar* string);
286
287 /**
288 * Gets the ASCII protocol output terminator string.
289 *
290 * @public @memberof GoEthernet
291 * @version Introduced in firmware 4.0.10.27
292 * @param ethernet GoEthernet object.
293 * @return A pointer to the terminator representing the ASCII protocol output delimiter.
294 */
295 GoFx(kChar*) GoEthernet_AsciiTerminator(GoEthernet ethernet);
296
297 /**
298 * Sets the ASCII protocol output terminator string.
299 *
300 * @public @memberof GoEthernet
301 * @version Introduced in firmware 4.0.10.27
302 * @param ethernet GoEthernet object.
303 * @param string A pointer to the string representing the ASCII protocol output terminator.
304 * @return Operation status.
305 */
306 GoFx(kStatus) GoEthernet_SetAsciiTerminator(GoEthernet ethernet, const kChar* string);
307
308 /**
309 * Gets the ASCII protocol output invalid value string.
310 *
311 * @public @memberof GoEthernet
312 * @version Introduced in firmware 4.0.10.27
313 * @param ethernet GoEthernet object.
314 * @return A pointer to the string representing the ASCII protocol output invalid value.
315 */
316 GoFx(kChar*) GoEthernet_AsciiInvalidValue(GoEthernet ethernet);
317
318 /**
319 * Sets the ASCII protocol output invalid value string.
320 *
321 * @public @memberof GoEthernet
322 * @version Introduced in firmware 4.0.10.27
323 * @param ethernet GoEthernet object.
324 * @param string A pointer to the string representing the ASCII protocol output invalid value.
325 * @return Operation status.
326 */
327 GoFx(kStatus) GoEthernet_SetAsciiInvalidValue(GoEthernet ethernet, const kChar* string);
328
329 /**
330 * Gets the ASCII protocol output custom data format string.
331 *
332 * @public @memberof GoEthernet
333 * @version Introduced in firmware 4.0.10.27
334 * @param ethernet GoEthernet object.
335 * @return A pointer to the string representing the ASCII protocol output custom data format.
336 */
337 GoFx(kChar*) GoEthernet_AsciiCustomDataFormat(GoEthernet ethernet);
338
339 /**
340 * Sets the ASCII protocol output custom data format string.
341 *
342 * @public @memberof GoEthernet
343 * @version Introduced in firmware 4.0.10.27
344 * @param ethernet GoEthernet object.
345 * @param string A pointer to the string representing the ASCII protocol output custom data format.
346 * @return Operation status.
347 */
348 GoFx(kStatus) GoEthernet_SetAsciiCustomDataFormat(GoEthernet ethernet, const kChar* string);
349
350 /**
351 * Enables or disables the ASCII protocol output custom data format.
352 *
353 * @public @memberof GoEthernet
354 * @version Introduced in firmware 4.0.10.27
355 * @param ethernet GoEthernet object.
356 * @param enabled kTRUE to enable custom data format output. kFALSE to use the default output format.
357 * @return Operation status.
358 */
359 GoFx(kStatus) GoEthernet_EnableAsciiCustomFormat(GoEthernet ethernet, kBool enabled);
360
361 /**
362 * Returns the value of whether the ASCII protocol custom data format is enabled or disabled.
363 *
364 * @public @memberof GoEthernet
365 * @version Introduced in firmware 4.0.10.27
366 * @param ethernet GoEthernet object.
367 * @return kTRUE if the custom data format is enabled. kFALSE otherwise.
368 */
369 GoFx(kBool) GoEthernet_AsciiCustomFormatEnabled(GoEthernet ethernet);
370
371 /**
372 * Enables or disables EthernetIP protocol output buffering.
373 *
374 * @public @memberof GoEthernet
375 * @version Introduced in firmware 4.0.10.27
376 * @param ethernet GoEthernet object.
377 * @param enabled kTRUE to enable buffering. kFALSE to disable it.
378 * @return Operation status.
379 */
380 GoFx(kStatus) GoEthernet_SetEIPBufferingEnabled(GoEthernet ethernet, kBool enabled);
381
382 /**
383 * Returns the value of whether the EthernetIP protocol output buffering is enabled or disabled.
384 *
385 * @public @memberof GoEthernet
386 * @version Introduced in firmware 4.0.10.27
387 * @param ethernet GoEthernet object.
388 * @return kTRUE if buffering is enabled. kFALSE otherwise.
389 */
390 GoFx(kBool) GoEthernet_EIPBufferingEnabled(GoEthernet ethernet);
391
392 /**
393 * Sets the EthernetIP protocol endian output type.
394 *
395 * @public @memberof GoEthernet
396 * @version Introduced in firmware 4.1.3.106
397 * @param ethernet GoEthernet object.
398 * @param type The endian output type to set.
399 * @return Operation status.
400 */
401 GoFx(kStatus) GoEthernet_SetEIPEndianOutputType(GoEthernet ethernet, GoEndianType type);
402
403 /**
404 * Returns the value of the EthernetIP protocol endian output type.
405 *
406 * @public @memberof GoEthernet
407 * @version Introduced in firmware 4.1.3.106
408 * @param ethernet GoEthernet object.
409 * @return Endian output type.
410 */
411 GoFx(kBool) GoEthernet_EIPEndianOutputType(GoEthernet ethernet);
412
413 /**
414 * Sets the EthernetIP protocol implicit trigger override.
415 *
416 * @public @memberof GoEthernet
417 * @version Introduced in firmware 4.2.4.7
418 * @param ethernet GoEthernet object.
419 * @param value The implicit trigger override value to set.
420 * @return Operation status.
421 */
422 GoFx(kStatus) GoEthernet_SetEIPImplicitTriggerOverride(GoEthernet ethernet, GoImplicitTriggerOverride value);
423
424 /**
425 * Returns the value of the EthernetIP protocol implicit trigger override.
426 *
427 * @public @memberof GoEthernet
428 * @version Introduced in firmware 4.2.4.7
429 * @param ethernet GoEthernet object.
430 * @return Implicit trigger override value.
431 */
432 GoFx(GoImplicitTriggerOverride) GoEthernet_EIPImplicitTriggerOverride(GoEthernet ethernet);
433
434 /**
435 * Enables or disables Modbus protocol output buffering.
436 *
437 * @public @memberof GoEthernet
438 * @version Introduced in firmware 4.0.10.27
439 * @param ethernet GoEthernet object.
440 * @param enabled kTRUE to enable buffering. kFALSE to disable it.
441 * @return Operation status.
442 */
443 GoFx(kStatus) GoEthernet_SetModbusBufferingEnabled(GoEthernet ethernet, kBool enabled);
444
445 /**
446 * Returns the value of whether Modbus protocol output buffering is enabled or disabled.
447 *
448 * @public @memberof GoEthernet
449 * @version Introduced in firmware 4.0.10.27
450 * @param ethernet GoEthernet object.
451 * @return kTRUE if buffering is enabled. kFALSE otherwise.
452 */
453 GoFx(kBool) GoEthernet_ModbusBufferingEnabled(GoEthernet ethernet);
454
455 kEndHeader()
456 #include <GoSdk/Outputs/GoEthernet.x.h>
457
458 #endif
k32u
GoEthernet::GoEthernet_ClearAllSources
kStatus GoEthernet_ClearAllSources(GoEthernet ethernet)
Removes (deselects) all selected sources for all possible ethernet output types.
GoEthernet::GoEthernet_SetEIPImplicitTriggerOverride
kStatus GoEthernet_SetEIPImplicitTriggerOverride(GoEthernet ethernet, GoImplicitTriggerOverride value)
Sets the EthernetIP protocol implicit trigger override.
GoEthernet::GoEthernet_AsciiCustomDataFormat
kChar * GoEthernet_AsciiCustomDataFormat(GoEthernet ethernet)
Gets the ASCII protocol output custom data format string.
GoEthernet::GoEthernet_ModbusBufferingEnabled
kBool GoEthernet_ModbusBufferingEnabled(GoEthernet ethernet)
Returns the value of whether Modbus protocol output buffering is enabled or disabled.
GoEthernet::GoEthernet_RemoveSource
kStatus GoEthernet_RemoveSource(GoEthernet ethernet, GoOutputSource type, kSize index)
Removes (deselects) the source at the specified index.
GoEthernet::GoEthernet_AsciiDataPort
k32u GoEthernet_AsciiDataPort(GoEthernet ethernet)
Gets the ASCII protocol data channel port number.
kSize
GoEthernet::GoEthernet_AsciiControlPort
k32u GoEthernet_AsciiControlPort(GoEthernet ethernet)
Gets the ASCII protocol control channel port number.
GoEthernet::GoEthernet_SetProtocol
kStatus GoEthernet_SetProtocol(GoEthernet ethernet, GoEthernetProtocol protocol)
Sets the protocol which will be output via ethernet.
GoEthernet::GoEthernet_SetAsciiHealthPort
kStatus GoEthernet_SetAsciiHealthPort(GoEthernet ethernet, k32u port)
Sets the port number of the ASCII health port.
GoEthernet::GoEthernet_SetAsciiDelimiter
kStatus GoEthernet_SetAsciiDelimiter(GoEthernet ethernet, const kChar *string)
Sets the ASCII protocol output delimiter string.
GoEthernetProtocol
Represents a ethernet output protocol.
GoEthernet::GoEthernet_TimeoutEnabled
kBool GoEthernet_TimeoutEnabled(GoEthernet ethernet)
Indicates whether the ethernet connection timeout is enabled.
GoEndianType
Represents an endian output type.
kChar
GoEthernet::GoEthernet_EIPImplicitTriggerOverride
GoImplicitTriggerOverride GoEthernet_EIPImplicitTriggerOverride(GoEthernet ethernet)
Returns the value of the EthernetIP protocol implicit trigger override.
GoEthernet::GoEthernet_AsciiDelimiter
kChar * GoEthernet_AsciiDelimiter(GoEthernet ethernet)
Gets the ASCII protocol output delimiter string.
GoEthernet::GoEthernet_SetAsciiCustomDataFormat
kStatus GoEthernet_SetAsciiCustomDataFormat(GoEthernet ethernet, const kChar *string)
Sets the ASCII protocol output custom data format string.
GoEthernet::GoEthernet_SetAsciiInvalidValue
kStatus GoEthernet_SetAsciiInvalidValue(GoEthernet ethernet, const kChar *string)
Sets the ASCII protocol output invalid value string.
GoEthernet::GoEthernet_Timeout
k64f GoEthernet_Timeout(GoEthernet ethernet)
Returns the connection timeout value in minutes.
GoEthernet::GoEthernet_SetAsciiControlPort
kStatus GoEthernet_SetAsciiControlPort(GoEthernet ethernet, k32u port)
Sets the port number of the ASCII control port.
GoEthernet::GoEthernet_AsciiOperation
GoAsciiOperation GoEthernet_AsciiOperation(GoEthernet ethernet)
Gets the ASCII protocol operational mode.
GoEthernet::GoEthernet_AddSource
kStatus GoEthernet_AddSource(GoEthernet ethernet, GoOutputSource type, k32u sourceId)
Selects the specified source for transmission.
GoSdkDef.h
Essential SDK declarations.
GoEthernet::GoEthernet_EnableTimeout
kStatus GoEthernet_EnableTimeout(GoEthernet ethernet, kBool value)
Enables or disables the ethernet connection timeout.
GoEthernet::GoEthernet_AsciiHealthPort
k32u GoEthernet_AsciiHealthPort(GoEthernet ethernet)
Gets the ASCII protocol health channel port number.
GoImplicitTriggerOverride
Represents an EthernetIP implicit messaging trigger override.
GoEthernet::GoEthernet_ClearSources
kStatus GoEthernet_ClearSources(GoEthernet ethernet, GoOutputSource type)
Removes (deselects) all selected sources for the specified output type.
GoEthernet::GoEthernet_SetTimeout
kStatus GoEthernet_SetTimeout(GoEthernet ethernet, k64f value)
Sets the connection timeout value.
GoOutputSource
Represents output sources.
GoEthernet::GoEthernet_EnableAsciiCustomFormat
kStatus GoEthernet_EnableAsciiCustomFormat(GoEthernet ethernet, kBool enabled)
Enables or disables the ASCII protocol output custom data format.
GoEthernet::GoEthernet_Protocol
GoEthernetProtocol GoEthernet_Protocol(GoEthernet ethernet)
Gets the protocol that the ethernet utilizes for output.
GoAsciiOperation
Represents an ASCII protocol operational type.
GoEthernet::GoEthernet_SetEIPBufferingEnabled
kStatus GoEthernet_SetEIPBufferingEnabled(GoEthernet ethernet, kBool enabled)
Enables or disables EthernetIP protocol output buffering.
GoEthernet::GoEthernet_OptionAt
k32u GoEthernet_OptionAt(GoEthernet ethernet, GoOutputSource type, kSize index)
Gets the source option at the specified index.
GoEthernet::GoEthernet_SetAsciiTerminator
kStatus GoEthernet_SetAsciiTerminator(GoEthernet ethernet, const kChar *string)
Sets the ASCII protocol output terminator string.
GoEthernet::GoEthernet_SetAsciiOperation
kStatus GoEthernet_SetAsciiOperation(GoEthernet ethernet, GoAsciiOperation mode)
Sets the ASCII operation mode.
kObject
kStatus
GoEthernet::GoEthernet_SourceAt
k32u GoEthernet_SourceAt(GoEthernet ethernet, GoOutputSource type, kSize index)
Gets the identifier of the selected output at the specified index.
GoEthernet::GoEthernet_SetModbusBufferingEnabled
kStatus GoEthernet_SetModbusBufferingEnabled(GoEthernet ethernet, kBool enabled)
Enables or disables Modbus protocol output buffering.
GoEthernet::GoEthernet_EIPEndianOutputType
kBool GoEthernet_EIPEndianOutputType(GoEthernet ethernet)
Returns the value of the EthernetIP protocol endian output type.
k64f
GoEthernet::GoEthernet_SetEIPEndianOutputType
kStatus GoEthernet_SetEIPEndianOutputType(GoEthernet ethernet, GoEndianType type)
Sets the EthernetIP protocol endian output type.
GoEthernet::GoEthernet_SetAsciiDataPort
kStatus GoEthernet_SetAsciiDataPort(GoEthernet ethernet, k32u port)
Sets the port number of the ASCII data port.
GoEthernet
Represents Ethernet output settings.
kBool
GoEthernet::GoEthernet_EIPBufferingEnabled
kBool GoEthernet_EIPBufferingEnabled(GoEthernet ethernet)
Returns the value of whether the EthernetIP protocol output buffering is enabled or disabled...
GoEthernet::GoEthernet_SourceCount
kSize GoEthernet_SourceCount(GoEthernet ethernet, GoOutputSource type)
Gets the number of sources of the specified output type that are currently selected for transmission...
GoEthernet::GoEthernet_OptionCount
kSize GoEthernet_OptionCount(GoEthernet ethernet, GoOutputSource type)
Gets the number of source options for the specified output type.
GoEthernet::GoEthernet_AsciiCustomFormatEnabled
kBool GoEthernet_AsciiCustomFormatEnabled(GoEthernet ethernet)
Returns the value of whether the ASCII protocol custom data format is enabled or disabled.
GoEthernet::GoEthernet_AsciiTerminator
kChar * GoEthernet_AsciiTerminator(GoEthernet ethernet)
Gets the ASCII protocol output terminator string.
GoEthernet::GoEthernet_AsciiInvalidValue
kChar * GoEthernet_AsciiInvalidValue(GoEthernet ethernet)
Gets the ASCII protocol output invalid value string.