Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
GoMaterial.h
Go to the documentation of this file.
1 /// @cond (Gocator_1x00 || Gocator_2x00)
2
3 /**
4 * @file GoMaterial.h
5 * @brief Declares the GoMaterial class.
6 *
7 * @internal
8 * Copyright (C) 2016 by LMI Technologies Inc.
9 * Licensed under the MIT License.
10 * Redistributed files must retain the above copyright notice.
11 */
12 #ifndef GO_MATERIAL_H
13 #define GO_MATERIAL_H
14
15 #include <GoSdk/GoSdkDef.h>
16
17 kBeginHeader()
18
19 /**
20 * @class GoMaterial
21 * @extends kObject
22 * @ingroup GoSdk
23 * @brief Represents configurable material acquisition settings.
24 */
25 typedef kObject GoMaterial;
26
27 /**
28 * Sets the material acquisition type.
29 *
30 * @public @memberof GoMaterial
31 * @version Introduced in firmware 4.1.3.106
32 * @param material GoMaterial object.
33 * @param type The material type to set.
34 * @return Operation status.
35 */
36 GoFx(kStatus) GoMaterial_SetType(GoMaterial material, GoMaterialType type);
37
38 /**
39 * Returns the user defined material acquisition type.
40 *
41 * @public @memberof GoMaterial
42 * @version Introduced in firmware 4.1.3.106
43 * @param material GoMaterial object.
44 * @return The material type.
45 */
46 GoFx(GoMaterialType) GoMaterial_Type(GoMaterial material);
47
48 /**
49 * Returns a boolean relating to whether the user defined material acquisition type value will be used by the system.
50 *
51 * @public @memberof GoMaterial
52 * @version Introduced in firmware 4.1.3.106
53 * @param material GoMaterial object.
54 * @return kTRUE if the user defined material type will be used and kFALSE otherwise.
55 */
56 GoFx(kBool) GoMaterial_IsTypeUsed(GoMaterial material);
57
58 /**
59 * Returns the material acquisition type to be used by the system.
60 *
61 * @public @memberof GoMaterial
62 * @version Introduced in firmware 4.1.3.106
63 * @param material GoMaterial object.
64 * @return The system value material type.
65 */
66 GoFx(GoMaterialType) GoMaterial_TypeSystemValue(GoMaterial material);
67
68 /**
69 * Sets the spot threshold.
70 *
71 * @public @memberof GoMaterial
72 * @version Introduced in firmware 4.1.3.106
73 * @param material GoMaterial object.
74 * @param value Spot threshold.
75 * @return Operation status.
76 */
77 GoFx(kStatus) GoMaterial_SetSpotThreshold(GoMaterial material, k32u value);
78
79 /**
80 * Returns the user defined spot threshold.
81 *
82 * @public @memberof GoMaterial
83 * @version Introduced in firmware 4.1.3.106
84 * @param material GoMaterial object.
85 * @return The spot threshold.
86 */
87 GoFx(k32u) GoMaterial_SpotThreshold(GoMaterial material);
88
89 /**
90 * Returns the minimum spot threshold limit.
91 *
92 * @public @memberof GoMaterial
93 * @version Introduced in firmware 4.1.3.106
94 * @param material GoMaterial object.
95 * @return The minimum spot threshold.
96 */
97 GoFx(k32u) GoMaterial_SpotThresholdLimitMin(GoMaterial material);
98
99 /**
100 * Returns the maximum spot threshold limit.
101 *
102 * @public @memberof GoMaterial
103 * @version Introduced in firmware 4.1.3.106
104 * @param material GoMaterial object.
105 * @return The maximum spot threshold.
106 */
107 GoFx(k32u) GoMaterial_SpotThresholdLimitMax(GoMaterial material);
108
109 /**
110 * Returns a boolean value representing whether the user specified spot threshold value is used.
111 *
112 * @public @memberof GoMaterial
113 * @version Introduced in firmware 4.1.3.106
114 * @param material GoMaterial object.
115 * @return kTRUE if it is used and kFALSE otherwise.
116 */
117 GoFx(kBool) GoMaterial_IsSpotThresholdUsed(GoMaterial material);
118
119 /**
120 * Returns the system spot threshold value.
121 *
122 * @public @memberof GoMaterial
123 * @version Introduced in firmware 4.1.3.106
124 * @param material GoMaterial object.
125 * @return The system spot threshold.
126 */
127 GoFx(k32u) GoMaterial_SpotThresholdSystemValue(GoMaterial material);
128
129 /**
130 * Sets the maximum spot width.
131 *
132 * @public @memberof GoMaterial
133 * @version Introduced in firmware 4.1.3.106
134 * @param material GoMaterial object.
135 * @param value Maximum spot width.
136 * @return Operation status.
137 */
138 GoFx(kStatus) GoMaterial_SetSpotWidthMax(GoMaterial material, k32u value);
139
140 /**
141 * Returns the user defined maximum spot width.
142 *
143 * @public @memberof GoMaterial
144 * @version Introduced in firmware 4.1.3.106
145 * @param material GoMaterial object.
146 * @return The maximum spot width.
147 */
148 GoFx(k32u) GoMaterial_SpotWidthMax(GoMaterial material);
149
150 /**
151 * Returns the maximum spot width minimum limit.
152 *
153 * @public @memberof GoMaterial
154 * @version Introduced in firmware 4.1.3.106
155 * @param material GoMaterial object.
156 * @return The maximum spot width minimum limit.
157 */
158 GoFx(k32u) GoMaterial_SpotWidthMaxLimitMin(GoMaterial material);
159
160 /**
161 * Returns the maximum spot width maximum limit.
162 *
163 * @public @memberof GoMaterial
164 * @version Introduced in firmware 4.1.3.106
165 * @param material GoMaterial object.
166 * @return The maximum spot width maximum limit.
167 */
168 GoFx(k32u) GoMaterial_SpotWidthMaxLimitMax(GoMaterial material);
169
170 /**
171 * Returns a boolean relating to whether the user defined spot width max value will be used by the system.
172 *
173 * @public @memberof GoMaterial
174 * @version Introduced in firmware 4.1.3.106
175 * @param material GoMaterial object.
176 * @return kTRUE if the user value will be used and kFALSE otherwise.
177 */
178 GoFx(kBool) GoMaterial_IsSpotWidthMaxUsed(GoMaterial material);
179
180 /**
181 * Returns the maximum spot width system value.
182 *
183 * @public @memberof GoMaterial
184 * @version Introduced in firmware 4.1.3.106
185 * @param material GoMaterial object.
186 * @return The maximum spot width system value.
187 */
188 GoFx(k32u) GoMaterial_SpotWidthMaxSystemValue(GoMaterial material);
189
190 /**
191 * Returns the number of spot selection type options.
192 *
193 * @public @memberof GoMaterial
194 * @version Introduced in firmware 4.3.3.124
195 * @param material GoMaterial object.
196 * @return The spot selection type option count.
197 */
198 GoFx(kSize) GoMaterial_SpotSelectionTypeOptionCount(GoMaterial material);
199
200 /**
201 * Returns the spot selection type option at the given index.
202 *
203 * @public @memberof GoMaterial
204 * @version Introduced in firmware 4.3.3.124
205 * @param material GoMaterial object.
206 * @param index The option list index to access.
207 * @return The spot selection type option at the given index.
208 */
209 GoFx(GoSpotSelectionType) GoMaterial_SpotSelectionTypeOptionAt(GoMaterial material, kSize index);
210
211 /**
212 * Sets the spot selection type.
213 *
214 * @public @memberof GoMaterial
215 * @version Introduced in firmware 4.1.3.106
216 * @param material GoMaterial object.
217 * @param type Spot selection type.
218 * @return Operation status.
219 */
220 GoFx(kStatus) GoMaterial_SetSpotSelectionType(GoMaterial material, GoSpotSelectionType type);
221
222 /**
223 * Returns the user defined spot selection type.
224 *
225 * @public @memberof GoMaterial
226 * @version Introduced in firmware 4.1.3.106
227 * @param material GoMaterial object.
228 * @return The maximum spot width.
229 */
230 GoFx(GoSpotSelectionType) GoMaterial_SpotSelectionType(GoMaterial material);
231
232 /**
233 * Returns a boolean relating to whether the user defined spot selection type will be used by the system.
234 *
235 * @public @memberof GoMaterial
236 * @version Introduced in firmware 4.1.3.106
237 * @param material GoMaterial object.
238 * @return kTRUE if the user value will be used and kFALSE otherwise.
239 */
240 GoFx(kBool) GoMaterial_IsSpotSelectionTypeUsed(GoMaterial material);
241
242 /**
243 * Returns the system spot selection type.
244 *
245 * @public @memberof GoMaterial
246 * @version Introduced in firmware 4.1.3.106
247 * @param material GoMaterial object.
248 * @return System spot selection type.
249 */
250 GoFx(GoSpotSelectionType) GoMaterial_SpotSelectionTypeSystemValue(GoMaterial material);
251
252 /**
253 * Sets the analog camera gain.
254 *
255 * @public @memberof GoMaterial
256 * @version Introduced in firmware 4.1.3.106
257 * @param material GoMaterial object.
258 * @param value Analog camera gain.
259 * @return Operation status.
260 */
261 GoFx(kStatus) GoMaterial_SetCameraGainAnalog(GoMaterial material, k64f value);
262
263 /**
264 * Returns the user defined analog camera gain value.
265 *
266 * @public @memberof GoMaterial
267 * @version Introduced in firmware 4.1.3.106
268 * @param material GoMaterial object.
269 * @return Analog camera gain value.
270 */
271 GoFx(k64f) GoMaterial_CameraGainAnalog(GoMaterial material);
272
273 /**
274 * Returns the analog camera gain minimum value limit.
275 *
276 * @public @memberof GoMaterial
277 * @version Introduced in firmware 4.1.3.106
278 * @param material GoMaterial object.
279 * @return Analog camera gain minimum value limit.
280 */
281 GoFx(k64f) GoMaterial_CameraGainAnalogLimitMin(GoMaterial material);
282
283 /**
284 * Returns the analog camera gain maximum value limit.
285 *
286 * @public @memberof GoMaterial
287 * @version Introduced in firmware 4.1.3.106
288 * @param material GoMaterial object.
289 * @return Analog camera gain maximum value limit.
290 */
291 GoFx(k64f) GoMaterial_CameraGainAnalogLimitMax(GoMaterial material);
292
293 /**
294 * Returns a boolean value representing whether the user defined analog camera gain is used.
295 *
296 * @public @memberof GoMaterial
297 * @version Introduced in firmware 4.1.3.106
298 * @param material GoMaterial object.
299 * @return kTRUE if the user defined analog camera gain is used and kFALSE otherwise.
300 */
301 GoFx(kBool) GoMaterial_IsCameraGainAnalogUsed(GoMaterial material);
302
303 /**
304 * Returns the analog camera gain system value.
305 *
306 * @public @memberof GoMaterial
307 * @version Introduced in firmware 4.1.3.106
308 * @param material GoMaterial object.
309 * @return The analog camera gain system value.
310 */
311 GoFx(k64f) GoMaterial_CameraGainAnalogSystemValue(GoMaterial material);
312
313 /**
314 * Sets the digital camera gain
315 *
316 * @public @memberof GoMaterial
317 * @version Introduced in firmware 4.1.3.106
318 * @param material GoMaterial object.
319 * @param value Digital camera gain.
320 * @return Operation status.
321 */
322 GoFx(kStatus) GoMaterial_SetCameraGainDigital(GoMaterial material, k64f value);
323
324 /**
325 * Returns the user defined digital camera gain value.
326 *
327 * @public @memberof GoMaterial
328 * @version Introduced in firmware 4.1.3.106
329 * @param material GoMaterial object.
330 * @return The digital camera gain system value.
331 */
332 GoFx(k64f) GoMaterial_CameraGainDigital(GoMaterial material);
333
334 /**
335 * Returns the digital camera gain minimum value limit.
336 *
337 * @public @memberof GoMaterial
338 * @version Introduced in firmware 4.1.3.106
339 * @param material GoMaterial object.
340 * @return Digital camera gain minimum value limit.
341 */
342 GoFx(k64f) GoMaterial_CameraGainDigitalLimitMin(GoMaterial material);
343
344 /**
345 * Returns the digital camera gain maximum value limit.
346 *
347 * @public @memberof GoMaterial
348 * @version Introduced in firmware 4.1.3.106
349 * @param material GoMaterial object.
350 * @return Digital camera gain maximum value limit.
351 */
352 GoFx(k64f) GoMaterial_CameraGainDigitalLimitMax(GoMaterial material);
353
354 /**
355 * Returns a boolean value representing whether the user's digital camera gain value is used by the system.
356 *
357 * @public @memberof GoMaterial
358 * @version Introduced in firmware 4.1.3.106
359 * @param material GoMaterial object.
360 * @return kTRUE if used and kFALSE otherwise.
361 */
362 GoFx(kBool) GoMaterial_IsCameraGainDigitalUsed(GoMaterial material);
363
364 /**
365 * Returns the system's digital camera gain value.
366 *
367 * @public @memberof GoMaterial
368 * @version Introduced in firmware 4.1.3.106
369 * @param material GoMaterial object.
370 * @return Digital camera gain system value.
371 */
372 GoFx(k64f) GoMaterial_CameraGainDigitalSystemValue(GoMaterial material);
373
374 /**
375 * Sets the dynamic sensitivity.
376 *
377 * @public @memberof GoMaterial
378 * @version Introduced in firmware 4.1.3.106
379 * @param material GoMaterial object.
380 * @param value Dynamic sensitivity.
381 * @return Operation status.
382 */
383 GoFx(kStatus) GoMaterial_SetDynamicSensitivity(GoMaterial material, k64f value);
384
385 /**
386 * Returns the user defined dynamic sensitivity value.
387 *
388 * @public @memberof GoMaterial
389 * @version Introduced in firmware 4.1.3.106
390 * @param material GoMaterial object.
391 * @return User defined dynamic sensitivity value.
392 */
393 GoFx(k64f) GoMaterial_DynamicSensitivity(GoMaterial material);
394
395 /**
396 * Returns the dynamic sensitivity minimum value limit.
397 *
398 * @public @memberof GoMaterial
399 * @version Introduced in firmware 4.1.3.106
400 * @param material GoMaterial object.
401 * @return Dynamic sensitivity minimum value limit.
402 */
403 GoFx(k64f) GoMaterial_DynamicSensitivityLimitMin(GoMaterial material);
404
405 /**
406 * Returns the dynamic sensitivity maximum value limit.
407 *
408 * @public @memberof GoMaterial
409 * @version Introduced in firmware 4.1.3.106
410 * @param material GoMaterial object.
411 * @return Dynamic sensitivity maximum value limit.
412 */
413 GoFx(k64f) GoMaterial_DynamicSensitivityLimitMax(GoMaterial material);
414
415 /**
416 * Returns a boolean representing whether the user defined dynamic sensitivity value is used.
417 *
418 * @public @memberof GoMaterial
419 * @version Introduced in firmware 4.1.3.106
420 * @param material GoMaterial object.
421 * @return kTRUE if used and kFALSE otherwise.
422 */
423 GoFx(kBool) GoMaterial_IsDynamicSensitivityUsed(GoMaterial material);
424
425 /**
426 * Returns the dynamic sensitivity system value.
427 *
428 * @public @memberof GoMaterial
429 * @version Introduced in firmware 4.1.3.106
430 * @param material GoMaterial object.
431 * @return Dynamic sensitivity system value.
432 */
433 GoFx(k64f) GoMaterial_DynamicSensitivitySystemValue(GoMaterial material);
434
435 /**
436 * Sets the dynamic threshold.
437 *
438 * @public @memberof GoMaterial
439 * @version Introduced in firmware 4.1.3.106
440 * @param material GoMaterial object.
441 * @param value Dynamic threshold.
442 * @return Operation status.
443 */
444 GoFx(kStatus) GoMaterial_SetDynamicThreshold(GoMaterial material, k32u value);
445
446 /**
447 * Returns the dynamic threshold minimum value limit.
448 *
449 * @public @memberof GoMaterial
450 * @version Introduced in firmware 4.1.3.106
451 * @param material GoMaterial object.
452 * @return Dynamic threshold minimum value limit.
453 */
454 GoFx(k32u) GoMaterial_DynamicThresholdLimitMin(GoMaterial material);
455
456 /**
457 * Returns the dynamic threshold maximum value limit.
458 *
459 * @public @memberof GoMaterial
460 * @version Introduced in firmware 4.1.3.106
461 * @param material GoMaterial object.
462 * @return Dynamic threshold maximum value limit.
463 */
464 GoFx(k32u) GoMaterial_DynamicThresholdLimitMax(GoMaterial material);
465
466 /**
467 * Returns the user defined dynamic threshold value.
468 *
469 * @public @memberof GoMaterial
470 * @version Introduced in firmware 4.1.3.106
471 * @param material GoMaterial object.
472 * @return The user defined dynamic threshold value.
473 */
474 GoFx(k32u) GoMaterial_DynamicThreshold(GoMaterial material);
475
476 /**
477 * Returns a boolean representing whether or not the user defined dynamic threshold is used by the system.
478 *
479 * @public @memberof GoMaterial
480 * @version Introduced in firmware 4.1.3.106
481 * @param material GoMaterial object.
482 * @return Dynamic threshold minimum value limit.
483 */
484 GoFx(kBool) GoMaterial_IsDynamicThresholdUsed(GoMaterial material);
485
486 /**
487 * Returns the dynamic threshold system value.
488 *
489 * @public @memberof GoMaterial
490 * @version Introduced in firmware 4.1.3.106
491 * @param material GoMaterial object.
492 * @return Dynamic threshold system value.
493 */
494 GoFx(k32u) GoMaterial_DynamicThresholdSystemValue(GoMaterial material);
495
496 /**
497 * Sets the gamma type.
498 *
499 * @public @memberof GoMaterial
500 * @version Introduced in firmware 4.1.3.106
501 * @param material GoMaterial object.
502 * @param value Gamma type.
503 * @return Operation status.
504 */
505 GoFx(kStatus) GoMaterial_SetGammaType(GoMaterial material, GoGammaType value);
506
507 /**
508 * Returns the user defined gamma type.
509 *
510 * @public @memberof GoMaterial
511 * @version Introduced in firmware 4.1.3.106
512 * @param material GoMaterial object.
513 * @return User defined gamma type.
514 */
515 GoFx(GoGammaType) GoMaterial_GammaType(GoMaterial material);
516
517 /**
518 * Returns a boolean representing whether the user defined gamma type is used by the system.
519 *
520 * @public @memberof GoMaterial
521 * @version Introduced in firmware 4.1.3.106
522 * @param material GoMaterial object.
523 * @return kTRUE if used and kFALSE otherwise.
524 */
525 GoFx(kBool) GoMaterial_IsGammaTypeUsed(GoMaterial material);
526
527 /**
528 * Returns the system's gamma type value.
529 *
530 * @public @memberof GoMaterial
531 * @version Introduced in firmware 4.1.3.106
532 * @param material GoMaterial object.
533 * @return The system gamma type value.
534 */
535 GoFx(GoGammaType) GoMaterial_GammaTypeSystemValue(GoMaterial material);
536
537 /**
538 * Enables or disables senstivity compensation. NOTE: This is only applicable to
539 * 2300 B series sensors.
540 *
541 * @public @memberof GoMaterial
542 * @version Introduced in firmware 4.3.3.124
543 * @param material GoMaterial object.
544 * @param value kTRUE to enable and kFALSE to disable.
545 * @return Operation status.
546 */
547 GoFx(kStatus) GoMaterial_EnableSensitivityCompensation(GoMaterial material, kBool value);
548
549 /**
550 * Returns the user defined sensitivity compensation value.
551 *
552 * @public @memberof GoMaterial
553 * @version Introduced in firmware 4.3.3.124
554 * @param material GoMaterial object.
555 * @return User defined sensitivity compensation.
556 */
557 GoFx(kBool) GoMaterial_SensitivityCompensationEnabled(GoMaterial material);
558
559 /**
560 * Returns a boolean representing whether the user defined sensitivity compensation is used by the system.
561 *
562 * @public @memberof GoMaterial
563 * @version Introduced in firmware 4.3.3.124
564 * @param material GoMaterial object.
565 * @return kTRUE if used and kFALSE otherwise.
566 */
567 GoFx(kBool) GoMaterial_IsSensitivityCompensationEnabledUsed(GoMaterial material);
568
569 /**
570 * Returns the system's sensitivity compensation value.
571 *
572 * @public @memberof GoMaterial
573 * @version Introduced in firmware 4.3.3.124
574 * @param material GoMaterial object.
575 * @return kTRUE if enabled and kFALSE otherwise.
576 */
577 GoFx(kBool) GoMaterial_SensitivityCompensationEnabledSystemValue(GoMaterial material);
578
579
580 kEndHeader()
581 #include <GoSdk/GoMaterial.x.h>
582
583 #endif
584
585 /// @endcond
k32u
GoMaterial::GoMaterial_SpotWidthMaxLimitMin
k32u GoMaterial_SpotWidthMaxLimitMin(GoMaterial material)
Returns the maximum spot width minimum limit.
GoMaterial::GoMaterial_SetSpotSelectionType
kStatus GoMaterial_SetSpotSelectionType(GoMaterial material, GoSpotSelectionType type)
Sets the spot selection type.
GoMaterial::GoMaterial_IsCameraGainDigitalUsed
kBool GoMaterial_IsCameraGainDigitalUsed(GoMaterial material)
Returns a boolean value representing whether the user's digital camera gain value is used by the syst...
GoMaterial::GoMaterial_TypeSystemValue
GoMaterialType GoMaterial_TypeSystemValue(GoMaterial material)
Returns the material acquisition type to be used by the system.
GoMaterial::GoMaterial_CameraGainDigitalSystemValue
k64f GoMaterial_CameraGainDigitalSystemValue(GoMaterial material)
Returns the system's digital camera gain value.
GoMaterial::GoMaterial_IsDynamicThresholdUsed
kBool GoMaterial_IsDynamicThresholdUsed(GoMaterial material)
Returns a boolean representing whether or not the user defined dynamic threshold is used by the syste...
GoMaterial::GoMaterial_SpotSelectionTypeSystemValue
GoSpotSelectionType GoMaterial_SpotSelectionTypeSystemValue(GoMaterial material)
Returns the system spot selection type.
GoMaterial::GoMaterial_SetSpotWidthMax
kStatus GoMaterial_SetSpotWidthMax(GoMaterial material, k32u value)
Sets the maximum spot width.
kSize
GoMaterial::GoMaterial_SpotThresholdLimitMax
k32u GoMaterial_SpotThresholdLimitMax(GoMaterial material)
Returns the maximum spot threshold limit.
GoMaterial
Represents configurable material acquisition settings.
GoMaterial::GoMaterial_CameraGainAnalogLimitMin
k64f GoMaterial_CameraGainAnalogLimitMin(GoMaterial material)
Returns the analog camera gain minimum value limit.
GoMaterial::GoMaterial_CameraGainDigital
k64f GoMaterial_CameraGainDigital(GoMaterial material)
Returns the user defined digital camera gain value.
GoMaterial::GoMaterial_SetSpotThreshold
kStatus GoMaterial_SetSpotThreshold(GoMaterial material, k32u value)
Sets the spot threshold.
GoMaterial::GoMaterial_CameraGainAnalogSystemValue
k64f GoMaterial_CameraGainAnalogSystemValue(GoMaterial material)
Returns the analog camera gain system value.
GoMaterial::GoMaterial_SetDynamicSensitivity
kStatus GoMaterial_SetDynamicSensitivity(GoMaterial material, k64f value)
Sets the dynamic sensitivity.
GoMaterialType
Represents a material acquisition type.
GoMaterial::GoMaterial_SpotThresholdSystemValue
k32u GoMaterial_SpotThresholdSystemValue(GoMaterial material)
Returns the system spot threshold value.
GoMaterial::GoMaterial_DynamicThresholdSystemValue
k32u GoMaterial_DynamicThresholdSystemValue(GoMaterial material)
Returns the dynamic threshold system value.
GoMaterial::GoMaterial_IsTypeUsed
kBool GoMaterial_IsTypeUsed(GoMaterial material)
Returns a boolean relating to whether the user defined material acquisition type value will be used b...
GoMaterial::GoMaterial_IsCameraGainAnalogUsed
kBool GoMaterial_IsCameraGainAnalogUsed(GoMaterial material)
Returns a boolean value representing whether the user defined analog camera gain is used...
GoMaterial::GoMaterial_SpotWidthMaxSystemValue
k32u GoMaterial_SpotWidthMaxSystemValue(GoMaterial material)
Returns the maximum spot width system value.
GoMaterial::GoMaterial_SensitivityCompensationEnabled
kBool GoMaterial_SensitivityCompensationEnabled(GoMaterial material)
Returns the user defined sensitivity compensation value.
GoSdkDef.h
Essential SDK declarations.
GoMaterial::GoMaterial_DynamicSensitivity
k64f GoMaterial_DynamicSensitivity(GoMaterial material)
Returns the user defined dynamic sensitivity value.
GoGammaType
Represents a material gamma type.
GoMaterial::GoMaterial_IsSpotWidthMaxUsed
kBool GoMaterial_IsSpotWidthMaxUsed(GoMaterial material)
Returns a boolean relating to whether the user defined spot width max value will be used by the syste...
GoMaterial::GoMaterial_SpotWidthMaxLimitMax
k32u GoMaterial_SpotWidthMaxLimitMax(GoMaterial material)
Returns the maximum spot width maximum limit.
GoMaterial::GoMaterial_DynamicSensitivityLimitMax
k64f GoMaterial_DynamicSensitivityLimitMax(GoMaterial material)
Returns the dynamic sensitivity maximum value limit.
GoMaterial::GoMaterial_SpotWidthMax
k32u GoMaterial_SpotWidthMax(GoMaterial material)
Returns the user defined maximum spot width.
GoMaterial::GoMaterial_SetDynamicThreshold
kStatus GoMaterial_SetDynamicThreshold(GoMaterial material, k32u value)
Sets the dynamic threshold.
GoMaterial::GoMaterial_GammaType
GoGammaType GoMaterial_GammaType(GoMaterial material)
Returns the user defined gamma type.
GoMaterial::GoMaterial_SpotSelectionTypeOptionCount
kSize GoMaterial_SpotSelectionTypeOptionCount(GoMaterial material)
Returns the number of spot selection type options.
GoMaterial::GoMaterial_SpotSelectionType
GoSpotSelectionType GoMaterial_SpotSelectionType(GoMaterial material)
Returns the user defined spot selection type.
GoMaterial::GoMaterial_SetCameraGainAnalog
kStatus GoMaterial_SetCameraGainAnalog(GoMaterial material, k64f value)
Sets the analog camera gain.
GoMaterial::GoMaterial_CameraGainDigitalLimitMin
k64f GoMaterial_CameraGainDigitalLimitMin(GoMaterial material)
Returns the digital camera gain minimum value limit.
GoMaterial::GoMaterial_SensitivityCompensationEnabledSystemValue
kBool GoMaterial_SensitivityCompensationEnabledSystemValue(GoMaterial material)
Returns the system's sensitivity compensation value.
GoMaterial::GoMaterial_SetType
kStatus GoMaterial_SetType(GoMaterial material, GoMaterialType type)
Sets the material acquisition type.
GoMaterial::GoMaterial_DynamicThresholdLimitMax
k32u GoMaterial_DynamicThresholdLimitMax(GoMaterial material)
Returns the dynamic threshold maximum value limit.
GoMaterial::GoMaterial_SpotThreshold
k32u GoMaterial_SpotThreshold(GoMaterial material)
Returns the user defined spot threshold.
GoMaterial::GoMaterial_DynamicThreshold
k32u GoMaterial_DynamicThreshold(GoMaterial material)
Returns the user defined dynamic threshold value.
GoMaterial::GoMaterial_GammaTypeSystemValue
GoGammaType GoMaterial_GammaTypeSystemValue(GoMaterial material)
Returns the system's gamma type value.
GoMaterial::GoMaterial_IsSpotThresholdUsed
kBool GoMaterial_IsSpotThresholdUsed(GoMaterial material)
Returns a boolean value representing whether the user specified spot threshold value is used...
GoMaterial::GoMaterial_IsSensitivityCompensationEnabledUsed
kBool GoMaterial_IsSensitivityCompensationEnabledUsed(GoMaterial material)
Returns a boolean representing whether the user defined sensitivity compensation is used by the syste...
kObject
GoMaterial::GoMaterial_SpotThresholdLimitMin
k32u GoMaterial_SpotThresholdLimitMin(GoMaterial material)
Returns the minimum spot threshold limit.
GoMaterial::GoMaterial_CameraGainAnalog
k64f GoMaterial_CameraGainAnalog(GoMaterial material)
Returns the user defined analog camera gain value.
kStatus
GoMaterial::GoMaterial_SetCameraGainDigital
kStatus GoMaterial_SetCameraGainDigital(GoMaterial material, k64f value)
Sets the digital camera gain.
GoMaterial::GoMaterial_CameraGainDigitalLimitMax
k64f GoMaterial_CameraGainDigitalLimitMax(GoMaterial material)
Returns the digital camera gain maximum value limit.
GoMaterial::GoMaterial_CameraGainAnalogLimitMax
k64f GoMaterial_CameraGainAnalogLimitMax(GoMaterial material)
Returns the analog camera gain maximum value limit.
GoSpotSelectionType
Represents a spot selection type.
k64f
GoMaterial::GoMaterial_IsGammaTypeUsed
kBool GoMaterial_IsGammaTypeUsed(GoMaterial material)
Returns a boolean representing whether the user defined gamma type is used by the system...
GoMaterial::GoMaterial_SetGammaType
kStatus GoMaterial_SetGammaType(GoMaterial material, GoGammaType value)
Sets the gamma type.
GoMaterial::GoMaterial_IsSpotSelectionTypeUsed
kBool GoMaterial_IsSpotSelectionTypeUsed(GoMaterial material)
Returns a boolean relating to whether the user defined spot selection type will be used by the system...
GoMaterial::GoMaterial_Type
GoMaterialType GoMaterial_Type(GoMaterial material)
Returns the user defined material acquisition type.
GoMaterial::GoMaterial_DynamicSensitivitySystemValue
k64f GoMaterial_DynamicSensitivitySystemValue(GoMaterial material)
Returns the dynamic sensitivity system value.
kBool
GoMaterial::GoMaterial_DynamicSensitivityLimitMin
k64f GoMaterial_DynamicSensitivityLimitMin(GoMaterial material)
Returns the dynamic sensitivity minimum value limit.
GoMaterial::GoMaterial_IsDynamicSensitivityUsed
kBool GoMaterial_IsDynamicSensitivityUsed(GoMaterial material)
Returns a boolean representing whether the user defined dynamic sensitivity value is used...
GoMaterial::GoMaterial_DynamicThresholdLimitMin
k32u GoMaterial_DynamicThresholdLimitMin(GoMaterial material)
Returns the dynamic threshold minimum value limit.
GoMaterial::GoMaterial_SpotSelectionTypeOptionAt
GoSpotSelectionType GoMaterial_SpotSelectionTypeOptionAt(GoMaterial material, kSize index)
Returns the spot selection type option at the given index.
GoMaterial::GoMaterial_EnableSensitivityCompensation
kStatus GoMaterial_EnableSensitivityCompensation(GoMaterial material, kBool value)
Enables or disables senstivity compensation.