Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
Public Member Functions
GoSetup Class Reference
GoSdk

## Description

Represents a device configuration.

Inheritance diagram for GoSetup:

## Public Member Functions
kStatus | GoSensor_Flush (GoSensor sensor)
| Initiates a sensor configuration, model file, and transformation synchronization if modifications are present. More...
k64f | GoSetup_ActiveAreaHeight (GoSetup setup, GoRole role)
| Gets the active area height. More...
k64f | GoSetup_ActiveAreaHeightLimitMax (GoSetup setup, GoRole role)
| Gets the maximum valid value for the ActiveAreaHeight setting. More...
k64f | GoSetup_ActiveAreaHeightLimitMin (GoSetup setup, GoRole role)
| Gets the minimum valid value for the ActiveAreaHeight setting. More...
k64f | GoSetup_ActiveAreaLength (GoSetup setup, GoRole role)
| Gets the active area Length. More...
k64f | GoSetup_ActiveAreaLengthLimitMax (GoSetup setup, GoRole role)
| Gets the maximum valid value for the ActiveAreaLength setting. More...
k64f | GoSetup_ActiveAreaLengthLimitMin (GoSetup setup, GoRole role)
| Gets the minimum valid value for the ActiveAreaLength setting. More...
k64f | GoSetup_ActiveAreaWidth (GoSetup setup, GoRole role)
| Gets the active area width. More...
k64f | GoSetup_ActiveAreaWidthLimitMax (GoSetup setup, GoRole role)
| Gets the maximum valid value for the ActiveAreaWidth setting. More...
k64f | GoSetup_ActiveAreaWidthLimitMin (GoSetup setup, GoRole role)
| Gets the minimum valid value for the ActiveAreaWidth setting. More...
k64f | GoSetup_ActiveAreaX (GoSetup setup, GoRole role)
| Gets the active area x origin. More...
k64f | GoSetup_ActiveAreaXLimitMax (GoSetup setup, GoRole role)
| Gets the maximum valid value for the ActiveAreaX setting. More...
k64f | GoSetup_ActiveAreaXLimitMin (GoSetup setup, GoRole role)
| Gets the minimum valid value for the ActiveAreaX setting. More...
k64f | GoSetup_ActiveAreaY (GoSetup setup, GoRole role)
| Gets the active area Y. More...
k64f | GoSetup_ActiveAreaYLimitMax (GoSetup setup, GoRole role)
| Gets the maximum valid value for the ActiveAreaY setting. More...
k64f | GoSetup_ActiveAreaYLimitMin (GoSetup setup, GoRole role)
| Gets the minimum valid value for the ActiveAreaY setting. More...
k64f | GoSetup_ActiveAreaZ (GoSetup setup, GoRole role)
| Gets the active area z origin. More...
k64f | GoSetup_ActiveAreaZLimitMax (GoSetup setup, GoRole role)
| Gets the maximum valid value for the ActiveAreaZ setting. More...
k64f | GoSetup_ActiveAreaZLimitMin (GoSetup setup, GoRole role)
| Gets the minimum valid value for the ActiveAreaZ setting. More...
kStatus | GoSetup_AddExposureStep (GoSetup setup, GoRole role, k64f exposure)
| Adds an exposure step. More...
kBool | GoSetup_AlignmentEncoderCalibrateEnabled (GoSetup setup)
| Gets the value of the post alignment encoder calibration setting. More...
GoAlignmentTarget | GoSetup_AlignmentMovingTarget (GoSetup setup)
| Gets the target type used for moving alignment calibration. More...
GoAlignmentTarget | GoSetup_AlignmentMovingTargetOptionAt (GoSetup setup, kSize index)
| Gets the moving alignment target option at the given index. More...
kSize | GoSetup_AlignmentMovingTargetOptionCount (GoSetup setup)
| Gets the moving alignment target option count. More...
GoAlignmentTarget | GoSetup_AlignmentStationaryTarget (GoSetup setup)
| Gets the target type used for stationary alignment calibration. More...
GoAlignmentTarget | GoSetup_AlignmentStationaryTargetOptionAt (GoSetup setup, kSize index)
| Gets the stationary alignment target option at the given index. More...
kSize | GoSetup_AlignmentStationaryTargetOptionCount (GoSetup setup)
| Gets the stationary alignment target option count. More...
GoAlignmentType | GoSetup_AlignmentType (GoSetup setup)
| Gets the type used for alignment calibration. More...
GoAlignmentType | GoSetup_AlignmentTypeOptionAt (GoSetup setup, kSize index)
| Gets the alignment type option at the given index. More...
kSize | GoSetup_AlignmentTypeOptionCount (GoSetup setup)
| Gets the alignment type option count. More...
kBool | GoSetup_AlignmentUsed (GoSetup setup)
| Indicates whether alignment can be used. More...
k32u | GoSetup_BackCameraHeight (GoSetup setup, GoRole role)
| Gets the camera region-of-interest height. More...
k32u | GoSetup_BackCameraUsed (GoSetup setup, GoRole role)
| Returns a boolean representing whether the back camera element is used. More...
k32u | GoSetup_BackCameraWidth (GoSetup setup, GoRole role)
| Gets the camera region-of-interest width. More...
k32u | GoSetup_BackCameraX (GoSetup setup, GoRole role)
| Gets the camera region-of-interest x origin. More...
k32u | GoSetup_BackCameraY (GoSetup setup, GoRole role)
| Gets the camera region-of-interest y origin. More...
k64f | GoSetup_BarHeight (GoSetup setup)
| Gets the height of the bar used for travel calibration. More...
kSize | GoSetup_BarHoleCount (GoSetup setup)
| Gets the number of holes that are defined on the calibration bar. More...
k64f | GoSetup_BarHoleDiameter (GoSetup setup)
| Gets the diameter of holes that are defined on the calibration bar. More...
k64f | GoSetup_BarHoleDistance (GoSetup setup)
| Gets the distance between holes that are defined on the calibration bar. More...
k64f | GoSetup_BarWidth (GoSetup setup)
| Gets the width of the bar used for travel calibration. More...
kStatus | GoSetup_ClearExposureSteps (GoSetup setup, GoRole role)
| Removes all exposure steps. More...
k64f | GoSetup_DiskDiameter (GoSetup setup)
| Gets the diameter of the disk used for travel calibration. More...
k64f | GoSetup_DiskHeight (GoSetup setup)
| Gets the height of the disk used for travel calibration. More...
k64f | GoSetup_DynamicExposureMax (GoSetup setup, GoRole role)
| Gets the maximum value for the Dynamic Exposure setting. More...
k64f | GoSetup_DynamicExposureMin (GoSetup setup, GoRole role)
| Gets the minimum value for the Dynamic Exposure setting. More...
kStatus | GoSetup_EnableAlignmentEncoderCalibrate (GoSetup setup, kBool enabled)
| Enables encoder calibration after alignment. More...
kStatus | GoSetup_EnableExternalInputZPulse (GoSetup setup, kBool enable)
| Sets the state of the external input triggered encoder Z-pulse feature. More...
kStatus | GoSetup_EnableInputTrigger (GoSetup setup, kBool enable)
| Sets the input trigger enabled state. More...
kStatus | GoSetup_EnableIntensity (GoSetup setup, kBool enable)
| Enables profile intensity collection. More...
kStatus | GoSetup_EnableMaxFrameRate (GoSetup setup, kBool enable)
| Enables or disables operation at full frame rate (ignoring frame rate setting). More...
kStatus | GoSetup_EnableOcclusionReduction (GoSetup setup, kBool enable)
| Sets the occlusion reduction enabled state. More...
kStatus | GoSetup_EnableTracking (GoSetup setup, GoRole role, kBool enable)
| Enables tracking. More...
kStatus | GoSetup_EnableTriggerGate (GoSetup setup, kBool enable)
| Sets the trigger gate feature. More...
kStatus | GoSetup_EnableUniformSpacing (GoSetup setup, kBool enable)
| Sets the user specified Uniform Spacing enabled state. More...
kStatus | GoSetup_EnableXDecimation (GoSetup setup, kBool enabled)
| Sets the status of x-direction decimation. More...
kStatus | GoSetup_EnableXGapFilling (GoSetup setup, kBool enable)
| Sets the status of x-direction gap-filling. More...
kStatus | GoSetup_EnableXMedian (GoSetup setup, kBool enabled)
| Sets the status of x-direction median. More...
kStatus | GoSetup_EnableXSlope (GoSetup setup, kBool enable)
| Sets the status of x-direction slope. More...
kStatus | GoSetup_EnableXSmoothing (GoSetup setup, kBool enabled)
| Sets the status of x-direction smoothing. More...
kStatus | GoSetup_EnableYDecimation (GoSetup setup, kBool enable)
| Sets the status of y-direction decimation. More...
kStatus | GoSetup_EnableYGapFilling (GoSetup setup, kBool enable)
| Sets the status of y-direction gap-filling. More...
kStatus | GoSetup_EnableYMedian (GoSetup setup, kBool enable)
| Sets the status of y-direction median. More...
kStatus | GoSetup_EnableYSlope (GoSetup setup, kBool enable)
| Sets the status of y-direction slope. More...
kStatus | GoSetup_EnableYSmoothing (GoSetup setup, kBool enable)
| Sets the status of y-direction smoothing. More...
k64f | GoSetup_EncoderSpacing (GoSetup setup)
| Gets the current encoder period for encoder-based triggering. More...
k64f | GoSetup_EncoderSpacingLimitMax (GoSetup setup)
| Constraint for the maximum valid value of the Encoder Period setting. More...
k64f | GoSetup_EncoderSpacingLimitMin (GoSetup setup)
| Constraint for the minimum valid value of the Encoder Period setting. More...
GoEncoderTriggerMode | GoSetup_EncoderTriggerMode (GoSetup setup)
| Gets the encoder trigger mode. More...
k64f | GoSetup_Exposure (GoSetup setup, GoRole role)
| Gets the exposure value. More...
k64f | GoSetup_ExposureLimitMax (GoSetup setup, GoRole role)
| Gets the maximum valid value for the Exposure setting. More...
k64f | GoSetup_ExposureLimitMin (GoSetup setup, GoRole role)
| Gets the minimum valid value for the Exposure setting. More...
GoExposureMode | GoSetup_ExposureMode (GoSetup setup, GoRole role)
| Gets the exposure mode. More...
GoExposureMode | GoSetup_ExposureModeOptionAt (GoSetup setup, GoRole role, kSize index)
| Gets the exposure mode option at the given index. More...
kSize | GoSetup_ExposureModeOptionCount (GoSetup setup, GoRole role)
| Gets the exposure mode option count. More...
k64f | GoSetup_ExposureStepAt (GoSetup setup, GoRole role, kSize index)
| Get the exposure step value specified by index. More...
kSize | GoSetup_ExposureStepCount (GoSetup setup, GoRole role)
| Get the number of exposure steps defined. More...
kBool | GoSetup_ExternalInputZPulseEnabled (GoSetup setup)
| Gets the state of the external input triggered encoder Z-pulse feature. More...
k64f | GoSetup_FrameRate (GoSetup setup)
| Reports the currently configured frame rate. More...
k64f | GoSetup_FrameRateLimitMax (GoSetup setup)
| Constraint for the maximum valid value of the Frame Rate setting. More...
k64f | GoSetup_FrameRateLimitMin (GoSetup setup)
| Constraint for the minimum valid value of the Frame Rate setting. More...
k32u | GoSetup_FrontCameraHeight (GoSetup setup, GoRole role)
| Gets the camera region-of-interest height. More...
k32u | GoSetup_FrontCameraWidth (GoSetup setup, GoRole role)
| Gets the camera region-of-interest width. More...
k32u | GoSetup_FrontCameraX (GoSetup setup, GoRole role)
| Gets the camera region-of-interest x origin. More...
k32u | GoSetup_FrontCameraY (GoSetup setup, GoRole role)
| Gets the camera region-of-interest y origin. More...
kBool | GoSetup_InputTriggerEnabled (GoSetup setup)
| Gets the input trigger enabled state. More...
kBool | GoSetup_InputTriggerEnabledSystemValue (GoSetup setup)
| Gets the input trigger system value. More...
kBool | GoSetup_InputTriggerEnabledUsed (GoSetup setup)
| Returns a boolean representing whether the user input trigger configuration is used. More...
kBool | GoSetup_IntensityEnabled (GoSetup setup)
| Reports whether the profile intensity collection is enabled. More...
kSize | GoSetup_IntensityStepIndex (GoSetup setup, GoRole role)
| Gets the intensity step index. More...
GoLayout | GoSetup_Layout (GoSetup setup)
| Gets the layout configuration module. More...
GoMaterial | GoSetup_Material (GoSetup setup, GoRole role)
| Gets the material acquisition module, used for material acquisition configuration. More...
kBool | GoSetup_MaxFrameRateEnabled (GoSetup setup)
| Reports whether or not system is configured to operate at full frame rate. More...
GoOcclusionReductionAlg | GoSetup_OcclusionReductionAlg (GoSetup setup)
| Gets the occlusion reduction algorithm. More...
kBool | GoSetup_OcclusionReductionAlgUsed (GoSetup setup)
| Returns a boolean representing whether the user occlusion reduction algorithm is used. More...
kBool | GoSetup_OcclusionReductionEnabled (GoSetup setup)
| Gets the occlusion reduction enabled state. More...
kBool | GoSetup_OcclusionReductionEnabledSystemValue (GoSetup setup)
| Gets the occlusion reduction system value. More...
kBool | GoSetup_OcclusionReductionEnabledUsed (GoSetup setup)
| Returns a boolean representing whether the user occlusion reduction configuration is used. More...
GoPartDetection | GoSetup_PartDetection (GoSetup setup)
| Gets the part detection module, used for part detection configuration. More...
GoPartMatching | GoSetup_PartMatching (GoSetup setup)
| Gets the part matching module, used for part matching configuration. More...
kSize | GoSetup_PatternSequenceCount (GoSetup setup, GoRole role)
| Gets the current pattern sequence count. More...
GoPatternSequenceType | GoSetup_PatternSequenceType (GoSetup setup, GoRole role)
| Gets the pattern sequence type. More...
GoPatternSequenceType | GoSetup_PatternSequenceTypeOptionAt (GoSetup setup, GoRole role, kSize index)
| Gets the pattern sequence type option at the given index. More...
kSize | GoSetup_PatternSequenceTypeOptionCount (GoSetup setup, GoRole role)
| Gets the pattern sequence type option count. More...
kBool | GoSetup_PatternSequenceTypeUsed (GoSetup setup, GoRole role)
| Returns a boolean value representing whether the pattern sequence type is used. More...
k64f | GoSetup_PlateHeight (GoSetup setup)
| Gets the height of the plate used for travel calibration. More...
kSize | GoSetup_PlateHoleCount (GoSetup setup)
| Gets the number of holes that are defined on the calibration plate. More...
k64f | GoSetup_PlateRefHoleDiameter (GoSetup setup)
| Gets the diameter of the reference hole defined on the calibration plate. More...
k64f | GoSetup_PlateSecHoleDiameter (GoSetup setup)
| Gets the diameter of the secondary hole defined on the calibration plate. More...
GoProfileGeneration | GoSetup_ProfileGeneration (GoSetup setup)
| Gets the profile generation module, used for profile generation configuration. More...
GoMode | GoSetup_ScanMode (GoSetup setup)
| Gets the default operation mode of the sensor system. More...
GoMode | GoSetup_ScanModeOptionAt (GoSetup setup, kSize index)
| Gets the scan mode option at the specified index. More...
kSize | GoSetup_ScanModeOptionCount (GoSetup setup)
| Gets the scan mode option count. More...
GoSections | GoSetup_Sections (GoSetup setup)
| Gets the Section configuration module, used for surface sections. More...
kStatus | GoSetup_SetActiveAreaHeight (GoSetup setup, GoRole role, k64f value)
| Sets the active area height. More...
kStatus | GoSetup_SetActiveAreaLength (GoSetup setup, GoRole role, k64f value)
| Sets the active area Length. More...
kStatus | GoSetup_SetActiveAreaWidth (GoSetup setup, GoRole role, k64f value)
| Sets the active area width. More...
kStatus | GoSetup_SetActiveAreaX (GoSetup setup, GoRole role, k64f value)
| Sets the active area x origin. More...
kStatus | GoSetup_SetActiveAreaY (GoSetup setup, GoRole role, k64f value)
| Sets the active area Y. More...
kStatus | GoSetup_SetActiveAreaZ (GoSetup setup, GoRole role, k64f value)
| Sets the active area z origin. More...
kStatus | GoSetup_SetAlignmentMovingTarget (GoSetup setup, GoAlignmentTarget target)
| Sets the target type used for moving alignment calibration. More...
kStatus | GoSetup_SetAlignmentStationaryTarget (GoSetup setup, GoAlignmentTarget target)
| Sets the target type used for stationary alignment calibration. More...
kStatus | GoSetup_SetAlignmentType (GoSetup setup, GoAlignmentType type)
| Sets the type used for alignment. More...
kStatus | GoSetup_SetBarHeight (GoSetup setup, k64f height)
| Sets the height of the bar used for travel calibration. More...
kStatus | GoSetup_SetBarHoleCount (GoSetup setup, kSize count)
| Sets the number of holes that are defined on the calibration bar. More...
kStatus | GoSetup_SetBarHoleDiameter (GoSetup setup, k64f diameter)
| Sets the diameter of holes that are defined on the calibration bar. More...
kStatus | GoSetup_SetBarHoleDistance (GoSetup setup, k64f distance)
| Sets the distance between holes that are defined on the calibration bar. More...
kStatus | GoSetup_SetBarWidth (GoSetup setup, k64f width)
| Sets the width of the bar used for travel calibration. More...
kStatus | GoSetup_SetDiskDiameter (GoSetup setup, k64f diameter)
| Sets the diameter of the disk used for travel calibration. More...
kStatus | GoSetup_SetDiskHeight (GoSetup setup, k64f height)
| Sets the height of the disk used for travel calibration. More...
kStatus | GoSetup_SetDynamicExposureMax (GoSetup setup, GoRole role, k64f exposure)
| Sets the maximum value for the Dynamic Exposure setting. More...
kStatus | GoSetup_SetDynamicExposureMin (GoSetup setup, GoRole role, k64f exposure)
| Sets the minimum value for the Dynamic Exposure setting. More...
kStatus | GoSetup_SetEncoderSpacing (GoSetup setup, k64f period)
| Sets the current encoder period for encoder-based triggering. More...
kStatus | GoSetup_SetEncoderTriggerMode (GoSetup setup, GoEncoderTriggerMode mode)
| Sets the encoder trigger mode. More...
kStatus | GoSetup_SetExposure (GoSetup setup, GoRole role, k64f exposure)
| Sets the exposure value. More...
kStatus | GoSetup_SetExposureMode (GoSetup setup, GoRole role, GoExposureMode mode)
| Sets the exposure mode. More...
kStatus | GoSetup_SetFrameRate (GoSetup setup, k64f frameRate)
| Sets the current frame rate for time-based triggering. More...
kStatus | GoSetup_SetIntensityStepIndex (GoSetup setup, GoRole role, kSize index)
| Sets the intensity step index. More...
kStatus | GoSetup_SetOcclusionReductionAlg (GoSetup setup, GoOcclusionReductionAlg alg)
| Sets the occlusion reduction algorithm. More...
kStatus | GoSetup_SetPatternSequenceType (GoSetup setup, GoRole role, GoPatternSequenceType type)
| Sets the pattern sequence type. More...
kStatus | GoSetup_SetPlateHeight (GoSetup setup, k64f height)
| Sets the height of the plate used for travel calibration. More...
kStatus | GoSetup_SetPlateHoleCount (GoSetup setup, kSize count)
| Sets the number of holes that are defined on the calibration plate. More...
kStatus | GoSetup_SetPlateRefHoleDiameter (GoSetup setup, k64f diameter)
| Sets the diameter of the reference hole defined on the calibration plate. More...
kStatus | GoSetup_SetPlateSecHoleDiameter (GoSetup setup, k64f diameter)
| Sets the diameter of the secondary hole defined on the calibration plate. More...
kStatus | GoSetup_SetScanMode (GoSetup setup, GoMode mode)
| Sets the default operation mode of the sensor system. More...
kStatus | GoSetup_SetSpacingIntervalType (GoSetup setup, GoRole role, GoSpacingIntervalType type)
| Sets the spacing interval type. More...
kStatus | GoSetup_SetTrackingAreaHeight (GoSetup setup, GoRole role, k64f height)
| Sets the tracking window height. More...
kStatus | GoSetup_SetTrackingSearchThreshold (GoSetup setup, GoRole role, k64f threshold)
| Sets the tracking window search threshold. More...
kStatus | GoSetup_SetTriggerDelay (GoSetup setup, k64f delay)
| Sets the trigger delay. More...
kStatus | GoSetup_SetTriggerSource (GoSetup setup, GoTrigger source)
| Sets the trigger source for profile triggering. More...
kStatus | GoSetup_SetTriggerUnit (GoSetup setup, GoTriggerUnits unit)
| Sets the system trigger units. More...
kStatus | GoSetup_SetXDecimationWindow (GoSetup setup, k64f window)
| Sets the x-direction decimation window. More...
kStatus | GoSetup_SetXGapFillingWindow (GoSetup setup, k64f window)
| Sets the status of x-direction gap-filling. More...
kStatus | GoSetup_SetXMedianWindow (GoSetup setup, k64f window)
| Sets the x-direction median window. More...
kStatus | GoSetup_SetXSlopeWindow (GoSetup setup, k64f window)
| Sets the status of x-direction slope. More...
kStatus | GoSetup_SetXSmoothingWindow (GoSetup setup, k64f window)
| Sets the x-direction smoothing window. More...
kStatus | GoSetup_SetXSubsampling (GoSetup setup, GoRole role, k32u xSubsampling)
| Sets the current x-resolution divider. More...
kStatus | GoSetup_SetYDecimationWindow (GoSetup setup, k64f window)
| Sets the y-direction decimation window. More...
kStatus | GoSetup_SetYGapFillingWindow (GoSetup setup, k64f window)
| Sets the y-direction gap-filling window. More...
kStatus | GoSetup_SetYMedianWindow (GoSetup setup, k64f window)
| Sets the y-direction median window. More...
kStatus | GoSetup_SetYSlopeWindow (GoSetup setup, k64f window)
| Sets the status of y-direction slope. More...
kStatus | GoSetup_SetYSmoothingWindow (GoSetup setup, k64f window)
| Sets the y-direction smoothing window. More...
kStatus | GoSetup_SetZSubsampling (GoSetup setup, GoRole role, k32u zSubsampling)
| Sets the current z-resolution divider. More...
k64f | GoSetup_SpacingInterval (GoSetup setup, GoRole role)
| Gets the spacing interval. More...
k64f | GoSetup_SpacingIntervalLimitMax (GoSetup setup, GoRole role)
| Gets the spacing interval value limit maximum. More...
k64f | GoSetup_SpacingIntervalLimitMin (GoSetup setup, GoRole role)
| Gets the spacing interval value limit minimum. More...
k64f | GoSetup_SpacingIntervalSystemValue (GoSetup setup, GoRole role)
| Gets the spacing interval system value. More...
GoSpacingIntervalType | GoSetup_SpacingIntervalType (GoSetup setup, GoRole role)
| Gets the spacing interval type. More...
kBool | GoSetup_SpacingIntervalTypeUsed (GoSetup setup, GoRole role)
| Gets the system value representing whether or not the user specified spacing interval type setting is being used at the moment. More...
kBool | GoSetup_SpacingIntervalUsed (GoSetup setup, GoRole role)
| Returns the state of whether the user specified spacing interval is used. More...
GoSurfaceGeneration | GoSetup_SurfaceGeneration (GoSetup setup)
| Gets the surface generation module, used for surface generation configuration. More...
GoTracheid | GoSetup_Tracheid (GoSetup setup, GoRole role)
| Gets the tracheid configuration module. More...
k64f | GoSetup_TrackingAreaHeight (GoSetup setup, GoRole role)
| Gets the tracking window height. More...
k64f | GoSetup_TrackingAreaHeightLimitMax (GoSetup setup, GoRole role)
| Gets the tracking window height maximum limit. More...
k64f | GoSetup_TrackingAreaHeightLimitMin (GoSetup setup, GoRole role)
| Gets the tracking window height minimum limit. More...
kBool | GoSetup_TrackingEnabled (GoSetup setup, GoRole role)
| Determines if tracking is enabled. More...
k64f | GoSetup_TrackingSearchThreshold (GoSetup setup, GoRole role)
| Gets the tracking window search threshold. More...
kBool | GoSetup_TrackingUsed (GoSetup setup, GoRole role)
| Returns a boolean value representing whether the Tracking Enabled field is used. More...
k64f | GoSetup_TransformedDataRegionHeight (GoSetup setup, GoRole role)
| Gets the transformed data region height value. More...
k64f | GoSetup_TransformedDataRegionLength (GoSetup setup, GoRole role)
| Gets the transformed data region length value. More...
k64f | GoSetup_TransformedDataRegionWidth (GoSetup setup, GoRole role)
| Gets the transformed data region width value. More...
k64f | GoSetup_TransformedDataRegionX (GoSetup setup, GoRole role)
| Gets the transformed data region X value. More...
k64f | GoSetup_TransformedDataRegionY (GoSetup setup, GoRole role)
| Gets the transformed data region Y value. More...
k64f | GoSetup_TransformedDataRegionZ (GoSetup setup, GoRole role)
| Gets the transformed data region Z value. More...
k64f | GoSetup_TriggerDelay (GoSetup setup)
| Gets the trigger delay. More...
k64f | GoSetup_TriggerDelayLimitMax (GoSetup setup)
| Reports the maximum trigger delay, based on current settings. More...
k64f | GoSetup_TriggerDelayLimitMin (GoSetup setup)
| Reports the minimum trigger delay, based on current settings. More...
kBool | GoSetup_TriggerGateEnabled (GoSetup setup)
| Reports whether the trigger gate feature is currently enabled. More...
kBool | GoSetup_TriggerGateEnabledSystemValue (GoSetup setup)
| Reports the trigger gate enabled system value. More...
kBool | GoSetup_TriggerGateEnabledUsed (GoSetup setup)
| Gets the system value representing whether or not the user specified trigger gate enabled setting is being used at the moment. More...
GoTrigger | GoSetup_TriggerSource (GoSetup setup)
| Gets the trigger source for profile triggering. More...
GoTriggerUnits | GoSetup_TriggerUnit (GoSetup setup)
| Gets the system trigger units. More...
kBool | GoSetup_UniformSpacingAvailable (GoSetup setup)
| Gets a boolean representing whether or not the user specified Uniform Spacing setting is being used at the moment. More...
kBool | GoSetup_UniformSpacingEnabled (GoSetup setup)
| Gets the user specified Uniform Spacing enabled state. More...
kBool | GoSetup_UniformSpacingEnabledSystemValue (GoSetup setup)
| Gets the Uniform Spacing enabled system value. More...
kBool | GoSetup_XDecimationEnabled (GoSetup setup)
| Gets the status of x-direction decimation. More...
kBool | GoSetup_XDecimationUsed (GoSetup setup)
| Indicates whether X decimation can be used for the current scan mode and device family. More...
k64f | GoSetup_XDecimationWindow (GoSetup setup)
| Gets the x-direction decimation window. More...
k64f | GoSetup_XDecimationWindowLimitMax (GoSetup setup)
| Gets the x-direction decimation window maximum. More...
k64f | GoSetup_XDecimationWindowLimitMin (GoSetup setup)
| Gets the x-direction decimation window minimum. More...
kBool | GoSetup_XGapFillingEnabled (GoSetup setup)
| Gets the status of x-direction gap-filling. More...
kBool | GoSetup_XGapFillingUsed (GoSetup setup)
| Indicates whether X gap filling can be used for the current scan mode and device family. More...
k64f | GoSetup_XGapFillingWindow (GoSetup setup)
| Gets the x-direction gap-filling window. More...
k64f | GoSetup_XGapFillingWindowLimitMax (GoSetup setup)
| Gets the x-direction gap-filling window maximum. More...
k64f | GoSetup_XGapFillingWindowLimitMin (GoSetup setup)
| Gets the x-direction gap-filling window minimum. More...
kBool | GoSetup_XMedianEnabled (GoSetup setup)
| Gets the status of x-direction median. More...
kBool | GoSetup_XMedianUsed (GoSetup setup)
| Indicates whether X median can be used for the current scan mode and device family. More...
k64f | GoSetup_XMedianWindow (GoSetup setup)
| Gets the x-direction median window. More...
k64f | GoSetup_XMedianWindowLimitMax (GoSetup setup)
| Gets the x-direction median window maximum. More...
k64f | GoSetup_XMedianWindowLimitMin (GoSetup setup)
| Gets the x-direction median window minimum. More...
kBool | GoSetup_XSlopeEnabled (GoSetup setup)
| Gets the status of x-direction slope. More...
kBool | GoSetup_XSlopeUsed (GoSetup setup)
| Indicates whether X slope can be used for the current scan mode and device family. More...
k64f | GoSetup_XSlopeWindow (GoSetup setup)
| Gets the x-direction slope window. More...
k64f | GoSetup_XSlopeWindowLimitMax (GoSetup setup)
| Gets the x-direction slope window maximum. More...
k64f | GoSetup_XSlopeWindowLimitMin (GoSetup setup)
| Gets the x-direction slope window minimum. More...
kBool | GoSetup_XSmoothingEnabled (GoSetup setup)
| Gets the status of x-direction smoothing. More...
kBool | GoSetup_XSmoothingUsed (GoSetup setup)
| Indicates whether X smoothing can be used for the current scan mode and device family. More...
k64f | GoSetup_XSmoothingWindow (GoSetup setup)
| Gets the x-direction smoothing window. More...
k64f | GoSetup_XSmoothingWindowLimitMax (GoSetup setup)
| Gets the x-direction smoothing window maximum. More...
k64f | GoSetup_XSmoothingWindowLimitMin (GoSetup setup)
| Gets the x-direction smoothing window minimum. More...
k32u | GoSetup_XSpacingCount (GoSetup setup, GoRole role)
| Gets the X spacing count. More...
k32u | GoSetup_XSubsampling (GoSetup setup, GoRole role)
| Gets the current x-resolution divider. More...
k32u | GoSetup_XSubsamplingOptionAt (GoSetup setup, GoRole role, kSize index)
| Gets the x-resolution option at the specified index. More...
kSize | GoSetup_XSubsamplingOptionCount (GoSetup setup, GoRole role)
| Gets the count of valid x-resolution options. More...
kBool | GoSetup_YDecimationEnabled (GoSetup setup)
| Gets the status of y-direction decimation. More...
kBool | GoSetup_YDecimationUsed (GoSetup setup)
| Indicates whether y decimation can be used for the current scan mode and device family. More...
k64f | GoSetup_YDecimationWindow (GoSetup setup)
| Gets the y-direction decimation window. More...
k64f | GoSetup_YDecimationWindowLimitMax (GoSetup setup)
| Gets the y-direction decimation window maximum. More...
k64f | GoSetup_YDecimationWindowLimitMin (GoSetup setup)
| Gets the y-direction decimation window minimum. More...
kBool | GoSetup_YGapFillingEnabled (GoSetup setup)
| Gets the status of y-direction gap-filling. More...
kBool | GoSetup_YGapFillingUsed (GoSetup setup)
| Indicates whether Y gap filling can be used for the current scan mode and device family. More...
k64f | GoSetup_YGapFillingWindow (GoSetup setup)
| Gets the y-direction gap-filling window. More...
k64f | GoSetup_YGapFillingWindowLimitMax (GoSetup setup)
| Gets the y-direction gap-filling window maximum. More...
k64f | GoSetup_YGapFillingWindowLimitMin (GoSetup setup)
| Gets the y-direction gap-filling window minimum. More...
kBool | GoSetup_YMedianEnabled (GoSetup setup)
| Gets the status of y-direction median. More...
kBool | GoSetup_YMedianUsed (GoSetup setup)
| Indicates whether Y median can be used for the current scan mode and device family. More...
k64f | GoSetup_YMedianWindow (GoSetup setup)
| Gets the y-direction median window. More...
k64f | GoSetup_YMedianWindowLimitMax (GoSetup setup)
| Gets the y-direction median window maximum. More...
k64f | GoSetup_YMedianWindowLimitMin (GoSetup setup)
| Gets the y-direction median window minimum. More...
kBool | GoSetup_YSlopeEnabled (GoSetup setup)
| Gets the status of y-direction slope. More...
kBool | GoSetup_YSlopeUsed (GoSetup setup)
| Indicates whether Y slope can be used for the current scan mode and device family. More...
k64f | GoSetup_YSlopeWindow (GoSetup setup)
| Gets the y-direction slope window. More...
k64f | GoSetup_YSlopeWindowLimitMax (GoSetup setup)
| Gets the y-direction slope window maximum. More...
k64f | GoSetup_YSlopeWindowLimitMin (GoSetup setup)
| Gets the y-direction slope window minimum. More...
kBool | GoSetup_YSmoothingEnabled (GoSetup setup)
| Gets the status of y-direction smoothing. More...
kBool | GoSetup_YSmoothingUsed (GoSetup setup)
| Indicates whether Y smoothing can be used for the current scan mode and device family. More...
k64f | GoSetup_YSmoothingWindow (GoSetup setup)
| Gets the y-direction smoothing window. More...
k64f | GoSetup_YSmoothingWindowLimitMax (GoSetup setup)
| Gets the y-direction smoothing window maximum. More...
k64f | GoSetup_YSmoothingWindowLimitMin (GoSetup setup)
| Gets the y-direction smoothing window minimum. More...
k32u | GoSetup_YSpacingCount (GoSetup setup, GoRole role)
| Gets the Y spacing count. More...
k32u | GoSetup_ZSubsampling (GoSetup setup, GoRole role)
| Gets the current z-resolution divider. More...
k32u | GoSetup_ZSubsamplingOptionAt (GoSetup setup, GoRole role, kSize index)
| Gets the z-resolution option at the specified index. More...
kSize | GoSetup_ZSubsamplingOptionCount (GoSetup setup, GoRole role)
| Gets the count of valid z-resolution options. More...

The documentation for this class was generated from the following files:

- GoSetup.h
- GoSensor.h